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Congratulations

You have just purchased a qualified baby monitor. Please read the instructions thoroughly before using the monitor system and keep it for future reference.

Content and Features

Items included in the package

Parent unit 

Baby unit 

2 adaptors: Out 5.5V/500mA

3 x AAA rechargeable batteries (1.2v, 600 mAh)
1 x user manual 
Baby Unit
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  1. Soft Antenna                          5. Belt Clip

  2. Sensitivity Control                     6. Hanging Hook

  3. Power Control / CHANNEL Switch:       7. Battery Compartment 
    OFF/ CH1/CH2                        8. Power Supply Socket

  4. Microphone   
Parent unit
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   1. Soft Antenna                           5. Belt Clip

   2. Volume Control                         6. Hanging Hook        

   3. Power Control / Channel Switch :         7. Battery Compartment   

     OFF/CH1/CH2                          8. Power Supply Socket

   4. Speaker

Main LCD Screen
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Adaptor:

The adaptors are low voltage power source that allow you to use your household electricity to run the Baby Monitor. Connect the adaptors to adaptor Jack in the Parents and Baby Unit. Both plug into any standard volt electrical outlet in your home. It is recommended to turn off the units before plug in or unplug the adaptors. 
CAUTION: These adaptors were made with a specific design for this product. They cannot be used with any other appliance. Never use a different type of adaptor with Baby Monitor.                                  
Important!

CAUTION

This product cannot replace responsible adult supervision.
This Baby Monitor is intended as an aid. Do not use it as a medical monitor or a substitute for responsible and proper adult supervision.
Make sure the baby unit and adaptor cable are always out of child's reach. Do not place the baby unit inside the baby's crib or playpen!
The antenna on the Units are fixed, do not try to extend them. Never attempt to modify the product.
Avoid using the product near water and expose to rain or moisture.
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Start-up

Setting the pilot tone

Press down the belt clip.
Open the battery compartment door.
Using the pilot tone changer in the battery compartment, you can choose between a total of 16 pilot tones. Ensure that the same setting is selected for both parent and baby units, otherwise a connection cannot be established.

Note: Change the pilot tone settings if there is interference from other devices such as baby monitors

or radios.
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Parent unit & baby unit Battery Installation

1. Open the battery compartment door.

2. Insert 3 x 1.5 V type AAA batteries into Parent unit & baby unit according to the +/- signs shown in the battery compartment, respectively.
4. Close battery compartment doors.

Battery Tips:

If the product is not in use for a long time, disconnect both units from the household electrical outlet. And remove the batteries or the exhausted batteries from the units, otherwise battery leakage and corrosion can damage them.
Dispose the batteries safely. 
Non-rechargeable battery is not to be recharged.
Rechargeable batteries are only to be charged under adult supervision.
CAUTION: Danger of explosion if battery is incorrectly replaced. Replace only with the batteries of the same and equivalent type.
Parent unit & baby unit Battery Charging. 

1.The supplied adaptors must be connected in order to charge the batteries. The battery level indicator shows that the device is charging.

2. As soon as the batteries are charged, the battery symbol appears complete in the display.

3. The charging process lasts for approx. 10 hours when the device is switched off.

Note:
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Please note that only the types of battery shown can be charged. The negative battery terminal must be stripped to approx. 7 mm (= without insulation).

Before the first use, the batteries should be fully charged. The charging process lasts for approx. 10 hours. The device offers an operation period of approx. 16 / 22 hours after this.

User can also install 3 alkaline A A A batteries instead of the supplied rechargeable batteries. Or directly operated by the supplied adaptors.

Help protect the environment

Batteries bearing one of the symbols shown opposite must not be disposed of in normal domestic waste.

[image: image8.jpg]& KKK




Instead take them to a collecting point for old batteries or special waste products (as your local authority for details) or return them to the dealer you bought them from. They will ensure batteries are disposed safely.

Testing Before First Time Usage

Test the baby unit emission and the mother unit reception.

Place baby unit and mother unit in room where you intend to use it. 

Set both baby unit and mother unit to the same channel (01 or 02) by switching the OFF/CH1/CH2 channel switch. Selected channel will be shown on the top right corner of the LCD screen.
NOTE: 

It is important that both units are in the same channel. Otherwise they can’t be connected with each other.
Baby unit emission:

1.  Push the switch for microphone sensitivity (’Sensitivity’) up or down in order to set

the desired noise sensitivity. If you have it set to high sensitivity, the baby unit transmits all noises.

2. As soon as the transmitter transmits a signal the “Baby calling ” icon will be flashed on the LCD screen and                                   the LCD backlight is activated. 
3. If the unit hears hardly any noise, it automatically switches to the energy saving mode. “Baby sleeping” icon shown on the LCD screen and the LCD backlight will be automatically turned off.

Parent unit reception:

1. Push the volume control (’Volume’) up or down in order to increase or reduce the receiver volume

on the parent unit.
2. If the unit receives a signal, the LCD backlight lights up automatically and the “Baby calling” icon flashes.
3. A few seconds after the unit receives no signals, the parent unit is automatically switched to energy saving mode. The “Baby sleeping” icon will be shown and the LCD backlight will be automatically turned off.

 Operation                     
• Position the baby unit so that it is in a raised position at a distance of 2 m from your baby.

• Switch the baby unit on by using the on / off / channel changer and select one of the two channels.

• The display will begin to light up and the selected channel is displayed.

• Switch the parent unit on by selecting the same channel as that set on the baby unit. The display will begin to light up and the selected channel is displayed.

Check the connection between the two devices

– the devices should not be more than a metre away from each other, or this may create feedback.

• If the baby unit is not transmitting any sound, the symbol ’baby is asleep’ appears and the backlight automatically switches to energy saving mode.

•If the baby unit is transmitting sounds, the symbols for ’baby is awake’ appears and the

backlight automatically switches on.

•If the connection between the two devices is cut off, Out of range alarm will be heard from the parent unit and out of range alarm icon appears.

Out of Range alarm and Range controls

Under below circumstances, out of range alarm will be heard from the parent unit and out of range alarm icon appears.

Parent unit is out of the range from baby unit.
The connection between baby unit and parent unit is cut off, such as the transmitter is turned off.

Baby unit is turned into a different channel to that of mother unit.

Baby unit or mother unit is working with a charger with low batteries.

Belt Clip

Baby unit or mother unit can both be carried around by using the belt clip provided on the back of each unit.
Trouble Shooting

	Problems
	Solutions

	1. No power.
	Unit is not turned on. Push the Unit OFF/CH1/CH2 switch to CHI or CH2 position 

Check if the batteries are installed properly. 

Make sure the adaptor is connected to the Unit properly if using the adaptor instead of batteries.

The Unit may be in low battery, change for new batteries.

	2. Message not Transmitted.           
	Sound sensitivity level of baby unitis too low, turn the

Sound Sensitivity level to proper position. 

Units are out of range or lost connection. Move baby unit closer to mother unit.

Ensure both units are in the same channel.

	3. Baby unit and parent unit do not show image.
	Power is turn off. Turn on both Units.

Check if both units are in the same channel.

Reposition or replace batteries.

	4. Hearing static or rustle from Baby unit.
	Baby unit is too near to parent unit and the volume is high . Increase the distance between baby unit and parent unit.

Reposition or replace batteries.


Technical Specifications

Power Supply Voltage:

Baby unit   – 3 AAA rechargeable batteries / alkaline batteries 

               & adaptor :  AC 100-240V – DC 5.5V 500mA
Parent unit   – 3 AAA rechargeable batteries / alkaline batteries 

               & adaptor :  AC 100-240V – DC 5.5V 500mA
Channel :    2 Channels & 16 Pilot Tone
Operation Frequency : CH1: 864.875 MHZ 

                     CH2: 864.925 MHZ

Operating Range: up to 800 metre in ideal conditions

Set includes: 1 baby unit, 1 parent unit, 3x AAA rechargeable batteries (for parent unit), 2 adaptors.

Battery icon:


  Full battery level


  Low battery level, reminds you to change the batteries


  Empty and flashing, batteries change is a must











Out of range alarm icon








Channel:CH01/CH02





“Baby sleeping”icon (energy saving mode)





“Baby calling”icon: constantly changing display








