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Congratulations

You have just purchased a qualified baby monitor. Please read the instructions thoroughly before using the monitor system and keep it for future reference.

Content and Features

Items included in the package

Parent unit 

Baby unit 

2 adaptors: Out 5.5V/500mA

3 x AAA rechargeable batteries (1.2v, 600 mAh)

1 x user manual 

Parents Unit：
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1.Power ON/OFF Key              2.Music Key  

3.PTT Key                        4.Volume “-” Key 

5.Microphone                     6.Power & Low battery indicator  

7. LCD display                    8.Volume “+” Key 

9.Night Light Key                  10.Speaker 

11.Belt Clip                       12.Night Light  

13.Battery  door                  14.USB Power Supply Socket
Baby Unit
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1.POWER ON/OFF Key            2.Music Key   

3.PAGE Key                      4.Volume “-” Key    
5.Microphone                     6.USB Power Supply Socket    

7.Power Indicator                 8.Night Light    

9.Volume “+” Key                 10.Night Light Key   

11.Speaker                      12.Temperature Detector             

13.Belt Clip                      14.Battery door
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LCD Display
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Adaptor:

The adaptors are low voltage power source that allow you to use your household electricity to run the Baby Monitor. Connect the adaptors to USB Power Supply Socket in the Parents and Baby Unit. Both plug into any standard volt electrical outlet in your home. It is recommended to turn off the units before plug in or unplug the adaptors. 
CAUTION: These adaptors were made with a specific design for this product. They cannot be used with any other appliance. Never use a different type of adaptor with Baby Monitor.  

Important!

CAUTION

This product cannot replace responsible adult supervision.
This Baby Monitor is intended as an aid. Do not use it as a medical monitor or a substitute for responsible and proper adult supervision.
Make sure the baby unit and adaptor cable are always out of child's reach. Do not place the baby unit inside the baby's crib or playpen!
The antenna on the Units are fixed, do not try to extend them. Never attempt to modify the product.
Avoid using the product near water and expose to rain or moisture.

Parent unit & baby unit Battery Installation

1. Open the battery compartment door by using a screw driver.

2. Insert 3 x 1.5 V type AAA batteries into Parent unit & baby unit according to the +/- signs shown in the battery compartment, respectively.
4. Close battery compartment doors.

Battery Tips:

If the product is not in use for a long time, disconnect both units from the household electrical outlet. And remove the batteries or the exhausted batteries from the units, otherwise battery leakage and corrosion can damage them.
Dispose the batteries safely. 
Non-rechargeable battery is not to be recharged.
Rechargeable batteries are only to be charged under adult supervision.
CAUTION: Danger of explosion if battery is incorrectly replaced. Replace only with the batteries of the same and equivalent type.
Parent unit Battery Charging (baby unit is non-rechargeable). 
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1.The supplied adaptors must be connected in order to charge the batteries. The battery level indicator shows that the device is charging.

2. As soon as the batteries are charged, the battery symbol appears complete in the display.

3. The charging process lasts for approx. 10 hours when the device is switched off.
Note:
Before the first use, the batteries should be fully charged. The charging process lasts for approx. 10 hours. The device offers an operation period of approx. 16 / 22 hours after this.

User can also install 3 alkaline A A A batteries instead of the supplied rechargeable batteries. Or directly operated by the supplied adaptors.

Help protect the environment

Batteries bearing one of the symbols shown opposite must not be disposed of in normal domestic waste.
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Instead take them to a collecting point for old batteries or special waste products (as your local authority for details) or return them to the dealer you bought them from. They will ensure batteries are disposed safely.
Operations Procedure of Parents 

Power ON/OFF 
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1>Insert 3 AAA batteries or connect the parents unit with the AC adaptor. The unit will be turned on automatically.
2>LCD will be fully displayed, 5 seconds for the backlight.
3>Power off by pressing POWER ON/OFF Key “Ⓘ” until no display on LCD.
  Volume Adjustment       

1>Press the key [image: image3.jpg]


 on the left side for decreasing volume level, a sound alert will be heard if up to the lowest.
2>Press the key [image: image4.jpg]


 on the right side for increasing volume level; a sound alert will be heard if up to the highest.
3>Totally 8 sound levels to indicate the volume. If no operation for 2 seconds, it will be returned to stand by status.

[image: image24.jpg]



[image: image25.jpg]


 Music Function (control the music songs of baby unit)
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1>Press music key    until music function is turned on. Meanwhile, the       songs No. will be showed in temperature area. If no operation on music key for 3 second, it will be returned to temperature display 
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2>Press music key    to choose the music order as follows, music１＞music２＞．．music 6>cycle
[image: image28.jpg]


3>Press music key    until turn off music function 
4>Exit music function during music playing by pressing “PTT” Key.

Night Light Function

1>Press night light key [image: image5.jpg]


 around 0.5 seconds, Night Light LED will be turned on. 
2>Press night light key [image: image6.jpg]


 around 0.5 seconds again, Night Light LED will be turned off.
3>Press night light key [image: image7.jpg]


 around 3 seconds, the night light of baby unit will be on. Meanwhile, night icon [image: image8.jpg]


 will be showed on LCD.
4>Press night light key [image: image9.jpg]


 around 3 seconds again, the night light of baby unit will be off. Meanwhile, night icon [image: image10.jpg]


 will be disappeared.

Talking Function 
1>Press PTT key to talk to the Baby unit.
2>Hold PTT key to continue talking.
3>Release PTT key to finish talking.

Remark: during talking, parent unit can’t receive any sound from baby unit. 
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Low Battery Indicator
1>When the unit is in low battery, the power indicator will be flashing which means the battery is low.
2>At the same time, “BI, BI” alert sound will be heard about 10 seconds one time.
3>The unit will be powered off when voltage is lower than 3.0V.
Out of Range Alert 
The parents unit will give out “BI, BI” sound alert which will be heard under such circumstances.
1>The units are detected out of communication range.
2>One of the parents and baby unit is in low battery or turned off.
Operations Procedure of Baby unit 

Power ON/OFF 

1>Insert 3 AAA batteries or connect the Baby unit with the AC adaptor. The unit will be turned on automatically.
2>Power indicator LED will be red.
3>Power off by pressing 3 seconds POWER ON/OFF Key until power indicator is off.
4>Power on again by pressing 3 seconds POWER ON/OFF Key.

Volume Adjustment       
1>Press the key [image: image11.jpg]


 on the left side for decreasing volume level, a sound alert will be heard if up to the lowest.
2>Press the key [image: image12.jpg]


 on the right side for increasing volume level; a sound alert will be heard if up to the highest.

  Music Function
1>Press the key “   ”on the right side to turn on/turn off the music.
2>Press the key “   ” to choose the music order as follows,music１＞music２＞．．music 6>cycle
3>Press music key until turning off the music function.
4>Or press PAGE key under the status of music playing to exit music function
  Baby Room Temperature Display
1>The temperature will be transmitted to parent unit after 30-60 seconds when powering on.
2>The temperature is influenced by the outer environment and will be changed accordingly.
  PAGE Function
1>Press PAGE key to call the PARENT unit.
2>The parent unit will give out “BI, BI” sound 10 times（BiBi..BiBi..BiBi）.
3>After 10 times, no sound will be heard unless pressing PAGE Key again.
Night Light Function.

1>Press night light key [image: image13.jpg]


 around 3 seconds, the night light of baby unit will be on
2>Press night light key [image: image14.jpg]


 around 3 seconds again, the night light of baby unit will be off.

Low Battery Indicator

When the unit is in low battery, the power indicator will be flashing which means the battery is low.

2>At the same time, “BI, BI” alert sound will be heard from parent unit until take out the batteries

form baby unit. The alert sound is about 10 seconds one time .
  3>The unit will be powered off when voltage is lower than 3.0V.
Communication.

Parent unit can receive the sound from baby unit when baby sound reaches 60dB.

Code Pairing
NOTE: the units were paired successfully in factory default .if not ,please operate according to following step.
1. Operate parent unit firstly: Turn off parent unit first and Turn on again, pressing PTT key and POWER OFF key “Ⓘ” 2 seconds at the same time (press the PTT key first and then press POWER OFF key “Ⓘ” ), power indicator will be alternatively flashing red and green lights. 

2. Then operate baby unit: Turn off baby unit first and Turn on again, pressing PAGE key and POWER OFF key 2 seconds at the same time ( press PAGE key first and then press POWER OFF key ), power indicator will be alternatively flashing red and green lights. 

3. One “BI” sound will be heard from both units after successful code pairing and power indicators will be turned to red.

Trouble shooting 

	Problems
	Solutions

	1. No power
	- Unit is turned off. 
- Check if the batteries are installed properly. 
- Make sure the adaptor is connected to the Unit properly if using the adaptor instead of batteries.
- The Unit may be in low battery status, change new batteries.

	2. Message not 

transmitted.



	- Units are out of range or lost connection. Ensure the distance between the units within communication range. 
Note: Communication range varies depending on surrounding 
conditions such as physical obstructions, interference.

- Make sure the PTT key of Parents unit is not pressed. 

- Ensure both units have paired successfully.

	3. No sound signal
	- Volume level on Parents unit is set too low. Adjust it to higher volume.
- Volume level of Baby unit is too low, Adjust it to higher volume.
- Units are out of range. Ensure the distance between the units within communication range.
- Make sure the PTT key of Parents unit is not pressed.
- Ensure both units have paired successfully.

	4. Received 

Conversation or 

sound from neighbors.

	- Signal interference due to other nursery monitor on the same ID Code or cordless phone used.

- Change both units to another ID code by repairing both units.

	5. Hearing static or rustle from Parent unit.
	- The both units are positioned too close to each other. Keep away two units at about 1m.

- The volume is set too high. Lower the volume of the Parent unit/baby unit.
- Reposition or replace batteries.

	6. Power indicator is flashing and can not receive or transmit 
	- The power is too low. Change new batteries or operated by the supplied adaptor.  


Technical Specifications
Power Supply Voltage:

Transmitter – 3 AAA rechargeable batteries / alkaline batteries 

            & adaptor :  AC 100V – 240V- DC 5.0V

Receiver   – 3 AAA rechargeable batteries / alkaline batteries 

            & adaptor :  AC 100V – 240V- DC 5.0V

Communication range(in open area)：≥300M；

Working temperature display：0~45℃；

Working frequency：2.400GHz～2.483GHz；

Mic Sensitivity : 1 to 2 meter



 �  Full battery level


� Low battery level, reminds you to change the batteries.


� Empty and flashing, batteries change is a must.
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