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USER MANUAL

DIGITAL BABY MONITOR

MODEL：BM-256

Congratulations

You have just purchased a qualified Wireless 2.4GHz Digital Baby Monitor. Please read this instruction carefully before using the product. Keep these instructions for future reference.
Safety Precautions
When using this unit, basic Safety Precautions should always be followed to reduce the risk of fire, electric shock, or personal injury.

Read and understand all instructions.
Follow all warnings and instructions marked on this unit or mentioned in this operation instruction.
The outer surface of the Baby Unit and Parent Unit can be cleaned with a cloth LIGHTLY dampened with water or a mild cleaning solution.
Never put the system near water, such as bathtub, bathroom sink, laundry tub, kitchen sink or in a wet basement, etc. Immersion of this unit in water could cause an electrical shock.

Place the unit securely on a stable surface. Serious damage and/or injury may result if the unit falls.
Do not cover slots and openings on the unit. They are provided for ventilation and protection against overheating.
To reduce the risk of electric shock, do not disassemble this unit. Take the unit to authorized service center or qualified technician who service or repair work is required. Opening or removing covers may expose you to dangerous voltages or other risks. Incorrect reassembly can cause electric shock when the unit is subsequently used.
Do keep the system away from heat sources such as radiators, heat registers, stoves or other appliances producing heat. Also keep these components out of direct sunlight.
Always unplug the AC adaptors if not using the system for long periods of time.

Caution: 
This product cannot replace responsible adult supervision. 
1．This Baby Monitor is intended as an aid. Do not use it as a medical monitor or a substitute for responsible and proper adult supervision. 
2．Make sure the Parents unit and adaptor cable are always out of child's reach. Do not place the Baby Unit inside the baby's crib or playpen!
WARNING: 

To reduce the risk of fire or electrical shock, do not expose this unit to rain or any type of moisture.

AC Adaptor:

The AC Adaptor is device that allows you to power on the system with your household electricity. The adaptor can be separately connected to DC IN connectors of Parent Unit and Baby Unit. Please be reminded to switch off the system before plugging or unplugging the adaptors.
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CAUTION: These adaptors are with exclusive design for this system. Please NEVER try to power up the system with different adaptors or use them for any other appliances。

Product Information
Parent Unit：
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Name
  1 — VOX Switch   2 —LCD Display    3a —Power Indicator  3b —Signal Strength Indicator  4 —Option Key (()          5 — Menu Key   6​ —Option Key (()  7 —PTT Switc   8 —Microphone   9 —Speaker  10 —Antenna               11 —On /Off & Volume Switch  12 —Adaptor Jack  13 — Battery Door           14 —Stand

Baby Unit:
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Name
1—Antenna  2—Night Vision Infrared LED’s  3—Thermal Via  4—On/Off Switc  5—Link Key  6—Microphone    

7—Camera 8—Camera  Adjusting  Knob  9—Mounting Clip  10—Compartment  11—ACAdaptorJack  12—Speaker  13—Hanging Hole  14—Foot Mat  15—Clip Hole

Operations Procedure of Parent Unit
Power ON/OFF
1> Remove screw by a screwdriver. Open the battery door.
2> Insert 3 AAA supplied rechargeable batteries into the Parent unit according to the polarity shown inside the battery compartment. Closed battery door and screw it up again, or connect the Parents unit with the AC adaptor. Power ON by turning the On/Off & Volume Switch until a click sound to be heard, Power Indicator will show red light and 3 second music will be heard.

3>Image will be displayed on LCD display if signal can be caught. Otherwise, white screen will be showed. 
4> Power off by turning off the Power Switch until a click sound to be heard, Red light of the power indicator will be off after 3 seconds, no display on LCD.

Volume Control

1> Increase the volume by turning up the VOL switch
2> Decrease the volume by turning down the VOL switch

Main Menu
Press MENU key to enter into main menu. Use (/( key to select, and press again MENU key to confirm.

Then, Select EXIT, Parent unit will return to LCD display. 
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Brightness 
1> Enter into main menu by pressing “MENU” key, press “(“or“(” key to select Brightness option, then confirm and enter into Brightness menu. 
2> Press (/( key to adjust the brightness level from 1 to 5. Press MENU key to confirm.

3> Select EXIT option and press “MENU” key to the live video.
Remarks: 1 – the darkest .5 – the brightest
Outdoor Mode

1> Enter into main menu by pressing “MENU” key, press “(“or“(” key to select Outdoor Mode option, then press MENU key to confirm and enter into Outdoor Mode menu. 
2> Press (/( key to turn on or turn off Outdoor Mode.，1 = Outdoor mode is turned on. 0= Outdoor mode is turned off.

Press MENU key to confirm.

3> Select EXIT option and press “MENU” key to the live video.
Remarks: Outdoor Mode is used when baby unit is placed in the outdoors.
Pairing 

1> For Parent Unit, enter into main menu by pressing “MENU” key, then press “(“or“(” key to select “Pairing” option and waiting.

2> For Baby Unit, press “Link” key 3 seconds until power indicator is fast flashing red light. Press “MENU” key of parent unit to confirm.  

3> When pairing successfully, parent unit will return to live video on its own. Meanwhile, both parent and baby unit will flash red light. 

If not, no display on LCD screen of parent unit. Pls repeat above steps.

Music Function

1> At the live video, press Option Key (() to turn on music.  

2> Press Option Key (() to choose the music order as follows, music１＞music２＞．．music 6>cycle
3> Press Option Key (() under the status of music playing to exit music function.
Remarks: Music function is not available under the status of main menu.

Talking Function
1> Under normal communicating, baby unit is transmitting sound and image to parent unit.

2> If parent unit need to talk back to baby unit, press PTT key of parent unit to talk.

3> Release PTT key to stop talking back to baby unit. The parent unit will be returned to receiving status.

VOX

When turning on VOX, transmission will be activated ONLY if sound is detected by Baby unit. LCD screen would be turned off if no sound is detected within 30 seconds. Once the sound is detected, it will automatically turn on the LCD screen. This is power saving feature.
Infrared Night Vision

When Baby unit is placed in dark environment, parent unit will be switched to Night Vision mode automatically. At this circumstance, parent unit can also receive image and sound. The image shows in black & white (See picture below.)
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Out of Range Alert.
Under below conditions, out of range alert can be heard from parent unit.

1> Baby unit is turned off.
2> The units are detected out of communication range.

3> Baby unit is in low power.

Screen Display

1> Signal Strength: 6 levels for signal strength, high level means stronger signal.
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2> Battery status: indicates the current battery status.
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Status can be: full charge, 3/4 charge, 2/4 charge, 1/4 charge, low battery.

Charging time: 8 hours with adaptor.
Antenna 

If parent unit is too far from baby unit and can’t receive good image from baby unit, here is an antenna helping to strength the signal. (See picture below.)
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Battery Installation
1. Remove screw by a screwdriver. 
2. Open the battery door. 

3. Insert 3 AA alkaline batteries(not included) into the Baby unit and 3 AAA alkaline or rechargeable batteries(included) into the Parent unit according to the polarity shown in the battery compartment.

4. Press down the screw and screw it up again.

5. Only one group of rechargeable battery equipped for parent unit, baby unit is supposed to be powered by adaptor..

Baby Unit  
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Parent Unit
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Charging the Batteries (only for Parent Unit)

Please charge the rechargeable batteries for first time usage. 
Use only the supplied AC adaptor for charging the assigned rechargeable batteries.

Plug into any nearby standard electrical outlet at home and charging automatically begins. A charging battery icon shows.

When fully charged, a full battery icon shows. The charging time for completely empty batteries at about 8 hours while the parent unit is turned off.

Battery Tips:

1>If the product is not in use for a long time, disconnect both units from the household electrical outlet. And remove the batteries or the exhausted batteries from baby unit, otherwise battery leakage and corrosion can damage them.

2>Dispose the battery safely.

3>Non-rechargeable battery is not be recharged. It may have a fire.

4>Rechargeable batteries are only to be charged under adult supervision. 

Privacy Protection

Always remember that you are using public airwaves when you use the Wireless 2.4GHz Digital Baby Monitor. Sound and video may be broadcasted to other receiving devices. Conversations, even from rooms near the camera, may be broadcast as well.

Operations Procedure of Baby Unit
Power ON/OFF
1> Remove screw by a screwdriver. Open the battery door.
2> Insert 3 AA alkaline batteries into the Baby unit according to the polarity shown in the battery compartment. Replace the battery door at the inclined angle, press down the screw and screw it up again; Or connect the Baby unit with AC adaptor. Power on by turning on the Power Switch, Power Indicator will flash and 3 seconds music will be heard.

3> Power off by turning off the Power Switch. All functions of baby unit will be stopped.
Lens Adjustment
If the video of the mother unit is blurred, adjust the lens switch of the baby unit until the video reaches the best image quality. (See picture below)
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Location and Set Up
You can position and adjust the Baby Unit in a variety of ways to provide the best view of your baby. To optimize the performance, position the Baby unit 3 ft (1m) away from the baby.

A. Set up removable Mounting Clip 
The Baby Unit can be clip on the table edge by setting up the removable mounting clip. After inserting the mounting clip at the base bottom, user can easily fix the Baby Unit into different location. Setting and disassembly method are shown in the figure below.
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B. Wall Mount

User can mount the baby unit or the parent unit at wall or ceiling by the wall mount hole. 
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Technical Specification

1>Frequency band：ISM；

2>Transmission rate；3Mbps

3>Communication mode：half-duplex；

4>Communication range(open area)：≥200M；

5>LCD：3.5"；

6>Transmission rate：320X240 dots(3.5")(receiver)

7>Focus：0.8m;visual range 60°(transmitter)

8>Operating temperature：0~45℃；

9>Power voltage (for parent unit)：3 X“AAA” rechargeable batteries / alkaline batteries

&adaptor : AC 100V – 240V- DC5.5V,800mA 

10>Power voltage (for baby unit)： 3 X“AA ”alkaline batteries；

 &adaptor : AC 100V – 240V- DC5.5V,800mA 

11>Working frequency：2.412～2.4694GHz；

12>Talking function: two way

Setting





Disassembly
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