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Congratulations

You have just purchased a qualified Wireless 2.4GHz Digital Baby Monitor. Please read this instruction carefully before using the product. Keep these instructions for future reference.
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Baby Unit:
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1- Camera lens        2- DC adaptor jack                 3-Microphone   

4- Speaker    5- Power (On/Off) Key         6- Pair Key  

Parent Unit：
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1 - Power (on/off)            2 – DC adaptor jack               3 - Belt clip                         4 - Power Indicator           5 - Menu key                     6 - Speaker            
7 - PTT Key                 8 –LCD screen                   9 – Option key （(）       

10- Option key（(）         11- Microphone

 Adaptor:

The Adaptor is device that allows you to power on the system with your household electricity. The adaptor can be separately connected to connectors of Parent Unit and Baby Unit. Please be reminded to switch off the system before plugging or unplugging the adaptors.
CAUTION: These adaptors are with exclusive design for this system. Please NEVER try to power up the system with different adaptors or use them for any other appliances.  

Safety Precautions
When using this unit, basic Safety Precautions should always be followed to reduce the risk of fire, electric shock, or personal injury.

Read and understand all instructions.

Follow all warnings and instructions marked on this unit or mentioned in this operation instruction.

This product is not intended to replace adult supervision but assistant tool. It is important that users should stay within the communication range of the system all the times when using it.

This product intended for indoor use only. Outdoor use may damage the system.
It is essential to check reception regularly. Please see the reception section for complete instructions.

Never put the system near water, such as bathtub, bathroom sink, laundry tub, kitchen sink or in a wet basement, etc. Immersion of this unit in water could cause an electrical shock.

Place the unit securely on a stable surface. Serious damage and/or injury may result if the unit falls.

Do not cover slots and openings on the unit. They are provided for ventilation and protection against overheating.

Install the unit where no one can step or trip on the cord.

Never push any objects through slots in this unit. This may result in the risk of fire or electric shock. Never spill any liquid on the unit.

To reduce the risk of electric shock, do not disassemble this unit. Take the unit to authorized service center or qualified technician when service or repair work is required. Opening or removing covers may expose you to dangerous voltages or other risks. Incorrect reassembly can cause electric shock when the unit is subsequently used.

Do keep the system away from heat sources such as radiators, heat registers, stoves or other appliances producing heat. Also keep these components out of direct sunlight.
Always unplug the adaptors if not using the system for long periods of time.
The outer surface of the Baby Unit and Parent Unit can be cleaned with a cloth LIGHTLY dampened with water or a mild cleaning solution.

WARNING: 

To reduce the risk of fire or electrical shock, do not expose this unit to rain or any type of moisture.

Privacy Protection

Always remember that you are using public airwaves when you use the Wireless 2.4GHz Digital Baby Monitor. Sound and video may be broadcasted to other receiving devices. Conversations, even from rooms near the camera, may be broadcasted as well.

CAUTION: To protect your privacy, always turn the system off when not in use. It is possible that the Parent Unit may be interfered from other devices in the 2.4GHz frequency range. 

Charging the Battery (only for Parent Unit) 
Parent unit is built in Li-ion rechargeable battery and baby unit is supposed to be powered by supplied adaptor. Please charge Parent Unit for the first time usage or when low battery icon is showed on the screen.

 Use only the supplied adaptor for charging the rechargeable battery.

 Plug into any nearby standard electrical outlet at home and charging automatically begins. A charging battery icon shows and red power indicator is on.

3. When fully charged, a full battery icon shows. The charging time for completely empty batteries is about 8 hours while the parent unit is turned off.

Reception Testing

Before using the Parent Unit or changing the location of the system, it is very important to test the video and sound reception:
To test the video reception

Place the Baby Unit in the most appropriate location. (e.g. on top of the table, mounting on the wall or ceiling) 

Focus and adjust the camera lens towards the baby. 
Check the video reception on screen of the Parent Unit and adjust the appropriate brightness level. (To adjust brightness, please see the “Functions Setup” section)
To test the sound quality

Speak in a whisper and with normal conversation sound level to Baby Unit.

Put the Parent Unit far away enough (at least 1m) from Baby Unit to prevent noise feedback.

Check the sound reception on speaker of the Parent Unit and adjust the appropriate volume. (To adjust volume, please see the “Functions Setup” section )
Functions Setup

Baby Monitor Functions Setup
A1. Power ON/OFF
Mother unit is built in Li-ion rechargeable battery. If there is not enough power, connect the Parents unit with the AC adaptor. Power ON by pressing Power Key until LCD is on. 

Connect the Baby unit with AC adaptor. Power on by pressing the Power Key until Power Indicator is on.

    Or insert 3 AA alkaline batteries into the Baby unit according to the polarity shown in the battery                                                                                       compartment and power on by pressing the Power Key until Power Indicator is on.
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3> Image will be displayed on LCD display if signal can be caught. Otherwise, below screen will be shown.
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4> Power off parent unit and baby unit by pressing the On/Off Key until red light of the power indicator is off and no display on LCD.

A2. Parent Unit Main Menu
Press MENU key to enter into main menu. Use (/( key to select, and press again FUN key to confirm. Then, press MENU key again or select EXIT, Parent unit will return to LCD display. 

[image: image10.png]



MAIN MENU

A2a. Brightness 

1> Enter into main menu by pressing “MENU” key, press (/( key to select Brightness option, then press “MENU” key to confirm. 
2> Press (/( key to adjust the brightness level from the darkest to the brightest (totally 4 levels). Press MENU key to confirm & return to main menu.
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Darkest                            brightest
Remarks: “( “ – minus the brightness   “(” – add the brightness
A2b. Volume  

1> Enter into main menu by pressing ““MENU”” key, press (/(key to select Volume option, then press “MENU” key to confirm. 
2> Press (/( key to minus/add the volume level from 1 to 4. Press “MENU” key to confirm & return to main menu.
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lowest                              loudest 

Remarks: “( “ – minus the volume level  “(” – add the volume level
A2c. Infrared Night Vision  

Enter into main menu by pressing ““MENU”” key, press (/( key to select “Night Vision” function option, then press “MENU” key again to confirm and enter into Night Vision menu.
Press (/( key to turn on/turn off night vision function. Press “MENU” key to confirm & return to main menu.
 Remark:

This is the “day” mode, night vision function is turned off.
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This is the “night”mode, night vision function is turned on.
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A2d. VOX  

Enter into main menu by pressing “MENU” key, press (/( key to select VOX function option, then press “MENU” key again to confirm.
Press (/( key to minus/add the VOX sensitivity from 1 to 4. Press Press “MENU” key to confirm & return to main menu.
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lowest sensitivity                     highest sensitivity

Remarks: Under VOX function, transmission will be activated ONLY if sound is detected by Baby unit. LCD screen would be turned off if no sound is detected as per the VOX sensitivity level. Once the sound is detected, it will automatically turn on the LCD screen. This is power saving feature.
A2e. Pairing 

For Parent Unit, enter into main menu by pressing “MENU” key, then press (/( key to select pairing option and waiting. See below.
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2> For Baby Unit, press “Link” key（at the back of baby unit) 4 seconds until power indicator flashing red light.
3> When pairing successfully, parent unit will return to live video on its own. Meanwhile, baby unit returns to stable red light. 

4> If not, no display on LCD screen of parent unit. Pls repeat above steps.

A2f. Exit 

When return to the live video from main menu, user can also select “EXIT” function option by pressing (/( key.
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B1. Parent Unit Screen Display

1> On the main screen of parent unit, the top left corner is signal strength indicator, the top right corner is the battery status and night vision icon.
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2> Battery status: indicates the current battery status of parent unit. 
[image: image6.jpg]


  [image: image7.jpg]


  [image: image8.jpg]


  [image: image9.jpg]



Status can be: full charge, 3/4 charge, 2/4 charge, 1/4 charge, low battery.

Charging time: 8 hours with adaptor.
B2. Talking Function (Two Way Communication)

1> Under normal communicating, baby unit is transmitting sound and image to parent unit.

2> If mother unit need to talk back to parent unit, press PTT key of parent unit to talk.

3> Release PTT key to stop talking back to baby unit. The parent unit will be returned to receiving status

B3. Out of Range Alert.

Under below conditions, out of range alert can be heard from parent unit.

a> Baby unit is turned off.
b> The units are detected out of communication range.
c> Baby unit is in low power.
Note: You can position and adjust the Baby Unit in a variety of ways to provide the best view of your baby. To optimize the performance, position the monitor unit 3 ft (1m) away from the baby.

Trouble Shooting
	Problem
	Possible Cause
	Solution

	Power indicator LED does not light up
	- Unit is not turned on.

- Power is switched off.
- Batteries may be used up.
- AC Adaptor not properly 
connected.


	- Press the Power Key to turn on it.
- Make sure that power outlet is turned on.

- Charge the battery/Replace new batteries.
- Check AC Adaptor jack-to-socket and 

plug-to-outlet connections.



	No image or sound or image blurred 
	- Wrong brightness level. 

- Set the video VOX ON and no sound is caught.

- Low volume level.
- Signal interference due to

other household appliance,

cordless or cellular 

telephone and etc.
	- Adjust the brightness to the desired level. 

- Press any key on the Parent unit to activate parent unit/ Select VOX Off/ give a sound to baby unit.

- Adjust volume level to the desired level.

- Press the LINK key of baby unit and select pairing option in main menu of parent unit to scan the channel. 

	Image flickers
	- Object is too closed to the Baby Unit.
- Baby or Parent Unit near 

metal concentration.

- Signal interference due to

other monitors, cordless or cellular telephones, etc.
	- Remove objects from the Baby Unit 

at about 1m.

- Test reception by moving the Baby Unit and / or Parent Unit to different locations throughout the house.

- Press the LINK key of baby unit and select pairing option in main menu of parent unit to scan the channel.

- Identify and eliminate the source of interference.

	Audio feedback 

(squealing)
	- Distance between two units are too closed.
- Volume is too high.


	- Keep away two units at about 1m.
- Lower the volume. 

	Dark image at Night
	- Power is switched off. 

- Batteries may be used up.
- Brightness level is too high / low.
	- Check the Baby Unit and/or Parent Unit power indicator.

- Check the connection of the adaptor 

and the Parent unit.

- Charge the battery/Replace new batteries.

- Adjust the Exposure level.


	Lose Link

(No signal)
	- Baby unit is turned off.

- The units are detected out of communication range.
- Baby unit is in low power.

	- Turn on the Baby unit.

- Ensure both units are in the 

communication range.

- Replace new batteries or operated by the supplied adaptor.


Technical Specification

Parent Unit

Operation voltage: DC 5V 1A or NI-MH 1.2V1000mAh x3 Battery. 

Temperature Range : 0℃～40℃ 

Power consumption : ≤2W 
Operation Frequency: 2.4GHz～2.4835GHz 
Max Range (clear line of sight) : up to 250m (in open area)

Resolution : 320(240 Pixel
Image Speed : > 12 films/second
LCD : 2.4” Color LCD 
Size of Hand Held : 102 x 29 x 69 mm 
Baby Unit

Operation voltage : DC 5V 1A (battery is not supported)

Power Output < 20 dBm
Temperature Range : 0℃～40℃
Power consumption : ≤3W
Operation Frequency : 2.4GHz～2.4835GHz 
Mic Sensitivity : 1 to 2 meter

Size of Baby Unit : 80 ( 80mm

Object Distance : 1-2m
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