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WIRELESS 2.4GHz DIGITAL BABY MONITOR
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Congratulations

You have just purchased a qualified Wireless 2.4GHz Digital Baby Monitor. Please read this instruction carefully before using the product. Keep these instructions for future reference.
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Parts and Quick Reference
Baby Unit:
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1—Night light +pairing key         2—Music key             3—Power indicator     

4—Signal strength indicator        5—Camera               6—Night light   

 7—Battery door                  8—Infrared sensor         9—On/Off Switch     

10— Adaptor Jack               11—Microphone           12—Speaker
Parent Unit:
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A. Name
  1— VOX Switch                     2—LCD Display           3a—Power Indicator  
3b—Signal strength indicator          4—Option key (()         5— Menu key   

 6​—Option key (()                   7—PTT Switch            8—Microphone  

 9—Speaker                        10 —Antenna              11—On /Off & volume switch       
12—Adaptor Jack                   13— Battery door          14—stand

AC Adaptor:
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The AC Adaptor is device that allows you to power on the system with your household electricity. The adaptor can be separately connected to DC IN connectors of Parent Unit and Baby Unit. Please be reminded to switch off the system before plugging or unplugging the adaptors.
CAUTION: These adaptors are with exclusive design for this system. Please NEVER try to power up the system with different adaptors or use them for any other appliances.  

Safety Precautions
When using this unit, basic Safety Precautions should always be followed to reduce the risk of fire, electric shock, or personal injury.

Read and understand all instructions.

Follow all warnings and instructions marked on this unit or mentioned in this operation instruction.

This product is not intended to replace adult supervision but assistant tool. It is important that users should stay within the communication range of the system all the times when using it.

This product intended for indoor use only. Outdoor use may damage the system.
It is essential to check reception regularly. Please see the reception section for complete instructions.

Never put the system near water, such as bathtub, bathroom sink, laundry tub, kitchen sink or in a wet basement, etc. Immersion of this unit in water could cause an electrical shock.

Place the unit securely on a stable surface. Serious damage and/or injury may result if the unit falls.

Do not cover slots and openings on the unit. They are provided for ventilation and protection against overheating.

Install the unit where no one can step or trip on the cord.

Never push any objects through slots in this unit. This may result in the risk of fire or electric shock. Never spill any liquid on the unit.

To reduce the risk of electric shock, do not disassemble this unit. Take the unit to authorized service center or qualified technician when service or repair work is required. Opening or removing covers may expose you to dangerous voltages or other risks. Incorrect reassembly can cause electric shock when the unit is subsequently used.

Do keep the system away from heat sources such as radiators, heat registers, stoves or other appliances producing heat. Also keep these components out of direct sunlight.
Always unplug the AC adaptors if not using the system for long periods of time.
The outer surface of the Baby Unit and Parent Unit can be cleaned with a cloth LIGHTLY dampened with water or a mild cleaning solution.

WARNING: 

To reduce the risk of fire or electrical shock, do not expose this unit to rain or any type of moisture.

Privacy Protection

Always remember that you are using public airwaves when you use the Wireless 2.4GHz Digital Baby Monitor. Sound and video may be broadcasted to other receiving devices. Conversations, even from rooms near the camera, may be broadcast as well.

CAUTION: To protect your privacy, always turn the system off when not in use. It is possible that the Parent Unit may be interfered from other devices in the 2.4GHz frequency range. 
Battery Installation

Installation
1. Remove screw by a screwdriver. 
2. Open the battery door. 

3. Insert 3 AAA alkaline batteries into the Baby unit and 3 AAA alkaline or rechargeable batteries into the Parent unit according to the polarity shown in the battery compartment.

4. Press down the screw and screw it up again.

Baby Unit 
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Parent Unit
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5. User can directly operate the unit by the supplied AC adaptor.
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( Use only the AC adaptor included supplied. 

( Unwrap and fully extend the AC adaptor cord. 

( Plug AC adaptor into a standard wall outlet.

( Wrap up and secure any excess AC adaptor cord.

Battery Tips:

- If the product is not in use for a long time, disconnect both units from the household electrical outlet. And remove the batteries or the exhausted batteries from baby unit, otherwise battery leakage and corrosion can damage them.

- Dispose the battery safely.

- Non-rechargeable battery is not be recharged. It may have a fire.

- Rechargeable batteries are only to be charged under adult supervision. 

Warning!

- The batteries shall not be exposed to excessive heat such as sunshine, fire or the like

- Danger of explosion if battery is incorrectly replaced. Dispose of used batteries according to the instructions. Replace only with the same and equivalent type.
Color Index of Power Indicator
	Indication
	Light Indicator

	
	Parent unit
	Baby unit

	Normal Operation
	Power indicator shows stable red light 
	Power indicator shows stable red light

	Low battery
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Red blank battery icon ”    ” shows on main screen  
	The right (last) LED indicator flashes green light

	In charging (Power Off)
	Power indicator shows stable green light
	N/A

	In charging(Power On)
	A charging battery icon shows on main screen
	

	Pairing status
	Select pairing option in main menu of parent unit
	The power indicator quick flashes green light.


Battery Status
Low battery status

Baby unit: When low battery, the right (last) LED indicator flashes green light. Please change the battery.
[image: image18.bmp]Parent unit: When low battery, red icon     will be shown on main screen of Parent unit. Please change the battery or charge the assigned rechargeable batteries.

Charging the Batteries (only for Parent Unit)

Please charge the rechargeable batteries for first time usage. 
Use only the supplied AC adaptor for charging the assigned rechargeable batteries.

Plug into any nearby standard electrical outlet at home and charging automatically begins. A charging battery icon shows.

When fully charged, a full battery icon shows. The charging time for completely empty batteries at about 8 hours while the parent unit is turned off.

SIMPLE to OPERATE

Just switch on the baby and parent units, and adjust the preferable sound level.

	1
	Connect with the AC Adaptor or install 3 x AAA alkaline batteries.
Insert 3xAAA batteries.                  With AC adaptor
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	2
	Turn on the Baby unit, then Parent unit.
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Remarks: Default setting: Paring is auto-scanned.

	3
	Adjust the appropriate volume level.
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Remarks: Night vision will be automatically switched when using in the dark, infra-red LED will be activated, and only Black & White image will be shown.


* For more detailed operation, please go to “Functions setup”
Reception Testing

Before using the Parent Unit or changing the location of the system, it is very important to test the video and sound reception:
To test the video reception

Place the Baby Unit in the most appropriate location. (e.g. on top of the table, mounting on the wall or ceiling) 

Focus the camera lens towards the baby. 
Check the video reception on screen of the Parent Unit and adjust the appropriate brightness level. (To adjust brightness, please see the “Functions Setup” section)
To test the sound quality

Speak in a whisper and with normal conversation sound level to Baby Unit.

Put the Parent Unit far away enough (at least 1m) from Baby Unit to prevent noise feedback.

Check the sound reception on speaker of the Parent Unit and adjust the appropriate volume. (To adjust volume, please see the “Functions Setup” section )
Functions Setup

Baby Monitor Functions Setup
A1. Power ON/OFF
Power on Parent unit by turning on the ON/Off & VOL Switch until a click sound to be heard, Power Indicator will show red light and 3 second music will be heard. Power on Baby unit by turning on the ON/Off Switch, Power LED and signal strength LED will flash and 3 second music will be heard.

Image will be displayed on LCD display if signal can be caught. Otherwise, white screen will be showed. 
Power off Parent unit by turning off the ON/Off & VOL Switch until a click sound to be heard, Red light of the power indicator will be off after 3 seconds, no display on LCD. Power off Baby unit by turning off the ON/Off Switch.
A2. Parent Unit Screen Display

1> Signal Strength: It shows the strength of the transmission signal of the transmit unit. 6 levels for signal strength, higher level means stronger signal.
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2> Parent unit Battery: indicates the current battery status.
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Status can be: full charge, 3/4 charge, 2/4 charge, 1/4 charge, low battery.

Charging time for completely empty batteries: at about 8 hours while the parent unit is turned off.

.

A3. Volume Control

1> Increase the volume by turning up the On/Off & Volume Switch
2> Decrease the volume by turning down On/Off & Volume Switch
A4. Main Menu
Press MENU key to enter into main menu. Use (/( key to select, and press again MENU key to confirm.

Then, Select EXIT, Parent unit will return to LCD display. 
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A4a. Color LED (LED sound strength indicator on Baby unit)
Under normal communicating, LED sound strength indicator on Baby unit will be flashing based on the sound volume. Lower volume will activate less indication lights. Otherwise, the louder the voice is, the more the flashing lights will be.
1> Enter into main menu by pressing “MENU” key, press “(“or“(” key to select Color LED, then confirm and enter into Color LED menu. 
2> Press (/( key to turn on / turn off the Color LED. 
1 = Baby Unit LED signal indicator “ON”

0 = Baby unit LED signal indicator “OFF”
Press MENU key to confirm.

3> Select EXIT and press “MENU” key to the live video.
A4b. Brightness 
1> Enter into main menu by pressing “MENU” key, press “(“or“(” key to select Brightness option, then confirm and enter into Brightness menu. 
2> Press (/( key to adjust the brightness level from 1 to 5. Press MENU key to confirm.

3> Select EXIT option and press “MENU” key to the live video.
Remarks: 1 – the darkest .5 – the brightest 
A4c. Night LED (Night Light of Parent Unit)

1> Enter into main menu by pressing “MENU” key, press “(“or“(” key to select Night LED option, then press MENU key to confirm and enter into Night LED menu. 
2> Press (/( key to turn on or turn off the Night LED. 
1 = Parent Unit Night Light “ON” 
0 = Parent unit Night Light “OFF”. 
Press MENU key to confirm.

3> Select EXIT option and press “MENU” key to the live video.
Besides controlled on Parent unit, night light can be also turned on / turned off by pressing “[image: image3.jpg]


”key of Baby unit.

A4d. Pairing 

1> For Parent Unit, enter into main menu by pressing “MENU” key, then press “(“or“(” key to select “Pairing” option and waiting.

2> For Baby Unit, press “[image: image4.jpg]


” key 3 seconds until power indicator LED is flashing. 

3> If pairing is successful, parent unit will return to live video on its own. Meanwhile, both power indicator lights of parent and baby unit will be on. 
4> If not, no display on LCD screen of parent unit. Pls repeat above steps.

Remark：Default setting: Paring is auto-scanned.

B. Other functions

B1. Music Function 
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1> At the live video, press “( “key to turn on music. 

2> Press the key“(” to choose the music order as follows, music１＞music２＞．．music 6> cycle
3> Press “(“ key when music play to exit music function.
Besides controlled on Parent unit, music function can be also turned on / turned off by pressing “[image: image5.jpg]


”key of Baby unit.

1> Press “[image: image6.jpg]


” key to turn on the music.

2> Press “[image: image7.jpg]


” key again to choose the music order as follows, music１＞music２＞．．music 6>cycle
3> Press “[image: image8.jpg]


“ key 4 seconds when music play to exit music function.
Remarks: Music function is not available under the status of main menu.

B2. Talking Function
1> Under normal communicating, baby unit is transmitting sound and image to parent unit.

2> If parent unit need to talk back to baby unit, press PTT key on parent unit to talk.

3> Release PTT key after talking. The parent unit will be returned to receiving status.

B3. VOX
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When turning on VOX, transmission will be activated ONLY if sound is detected by Baby unit. LCD screen would be turned off if no sound is detected within 30 seconds. Once the sound is detected, it will automatically turn on the LCD screen. This is power saving feature.
B4. Infrared Night Vision

When Baby unit is placed in dark environment, parent unit will be switched to Night Vision mode automatically. At this circumstance, parent unit can also receive image and sound. The image shows in black & white (See picture below.)
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B5. Out of Range Alert.

Under below conditions, out of range alert can be heard from parent unit.

a> Baby unit is turned off.
b> The units are detected out of communication range.
c> Baby unit is in power low.
B6. Antenna 

If parent unit is too far from baby unit and can’t receive good image from baby unit, here is an antenna helping to strength the signal. (See picture below.)
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Trouble Shooting

	Problem
	Possible Cause
	Solution

	Power indicator LED does not light up
	- Unit is not turned on.
- Power is switched off

- Batteries may be used up

- AC Adaptor not properly 
connected.
	- Slide the ON/OFF switch to the “ON” position

- Make sure that power outlet is turned on.

- Replace new batteries

- Check AC Adaptor jack-to-socket and 

plug-to-outlet connections.

	No image or sound
	- Wrong exposure level 

- Mode may be set to Video off /Sleep

- Maybe be set VOX ON

- Low volume level

- Signal interference due to

other household appliance,

cordless or cellular 

telephone and etc.
	- Adjust the exposure to the desired level. 

- Set the Parent unit to Normal mode.

- Press any key on the Parent unit to turn into Normal mode / Select no timeout / VOX Off
- Adjust volume level to the desired level.

- Press the [image: image11.jpg]


 key of baby unit and select pairing option in main menu of parent unit to pair again. 

	Image flickers
	- Object is too closed to the Baby Unit

- Baby or Parent Unit near 

metal concentration.

- Signal interference due to

other monitors, cordless or cellular telephones, etc.


	- Remove objects from the Baby Unit 

at about 1m.

- Test reception by moving the Baby Unit and / or Parent Unit to different locations throughout the house.

- Press the [image: image12.jpg]


 key of baby unit and select pairing option in main menu of parent unit to pair again.. 

- Identify and eliminate the source of interference.



	Audio feedback 

(squealing)
	- Distance between two units are too closed

- Volume is too high.


	- Keep away two units at about 1m

- Lower the volume 

	Dark image at Night
	- Power is switched off 

-Batteries may be used up.

- Exposure level is too high / low
	- Check the Baby Unit and/or Parent Unit power indicator.

- Check the connection of the adaptor 

and the Parent unit.

- Replace new batteries.

- Adjust the Exposure level



	Lose Link

(No signal)
	- Wrong channel

- Baby unit is turned off.

- The units are detected out of communication range
- Baby unit is in low power.

	- Ensure both units have already scanned 

the corresponding channel.

- Turn on the Baby unit.

- Ensure both units are in the 

communication range.

- Replace new batteries or operated by the supplied adaptor.


Technical Specification

Parent Unit

operation voltage: DC 5.5V 800mA or 3 x “AAA” rechargeable/ alkaline batteries 

Temperature Range : 0℃～40℃ 

Power consumption : ≤4W 

Operation Frequency: 2.4GHz～2.4835GHz 
Max Range (clear line of sight) : up to 250m (in open area)

Resolution : 320(240 Pixel

Image Speed : < 12 films/second

LCD : 3.5” Color LCD 

Size of Hand Held : 120 x 28 x 90 mm 
Baby Unit

Operation voltage : DC5.5V 800mA or 3 x “AAA” alkaline batteries

Power Output : 20 dBm

Temperature Range : 0℃～40℃
Power consumption : ≤4W

Operation Frequency : 2.4GHz～2.4835GHz 
Mic Sensitivity : 1 to 2 meter

Size of Baby Unit : 129 ( 88 x 83mm

Object Distance : 1-2m
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