
Instruction Manual Model Number WT-548

Buttons and Controls
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Main Screen Instructions
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1. VOX 

2. Roger Beep 

3. Channel scan

4. Tansmitting mode (TX) or Receiving mode (RX)

5. Channel number: displays current channel

6. Key lock indicator

7. Subcode

8. Battery level indicator   
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low battery:      display battery icon without blinking, reminder to change or charge battery           
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Charging:      battery icon blinking

Remark:
All the icon will be displayed on the LCD screen for 1 second when the radio be turned on with battery

Other Features of Various Symbols Shown on the LCD
	Symbol
	Major feature
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	Channel Selection
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	Subcode Selection
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	VOX Voice Activation
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	Auto-scan of Channel
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	Monitor Function
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	Call Tone Selecton
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	Key Beep
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	Roger Beep
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	Power Selecton


Battery Installation

1. Switch off the radio and remove the belt clip
2. Open the battery compartment door 
3. Insert batteries according to the anode-cathode signs shown inside battery compartment. Close the battery compartment door. Press and rotate the belt clip to its nomal position

Note:

1. Don’t mix new and old, different styles, alkaline and rechargeable and different capacity battery.
2. There is a danger of explosion if battery is incorrectly replaced. Replaced only with the same or equivalent type.
3. Attention should be drawn to the environmental aspects of battery disposal.

4. To avoid battery leakage, remove batteries if it is not used for a long time.
5. When the batteries are damaged, please disregard and dispose them with care. Do not dispose of the batteries to heat source to avoid explosion.
Recharging Function

Low Battery Alert
When the battery level becomes low, the battery icon blinks on the screen with alarm. When the battery is too low, the unit will power off automatically.
Voltage under 3.25V is undervoltage, the unit will power off automatically when voltage under 3.2V.
Please change the batteries. If you use NIMH rechargeable, please used supplied charging adaptor for charging. Please do not charge it over 8 hours or the unit may not function properly.
Use charging adaptor for charging: 
   Connect the adaptor side into socket and connect the charging jack hole at the top of the unit, you can charge two units at the same time.Battery icon appears on the LCD when the unit is in charging. Battery icon disappears when the unit is fully charged after 8 hours.
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    Charging when unit is turned off      Charging when unit is turned on

Note:

☆ Please fully charge the rechargeable batteries before first time usage.
☆ This is a danger of explosion or product damage if Alkaline batteries is placed inside battery compartment for charging.
☆ Please use only the supplied rechargeable batteries, AC/DC adaptors for charging, otherwise may damage the unit or may cause explosion.

☆ When the unit is power on and charging, PTT and CALL key is not activate.

Quick Start

A． Power On / Off
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1.  Power On: Press and hold    key for 2 seconds to power on the radio; Meanwhile there is a “Beep” sound to indicate the unit is power on.
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2.  Power Off: Press again    for 2 seconds during standby operation to turn off the radio, A “Bi” sound will also be heard, indicating the radio is going to be switched off.
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Remarks: When the walkie talkie is connected with the power supply, it will power on automatically.
B. Volume Level Adjustment
1. Press UP or DOWN key to select the volume level from 01 to 07(Fig 4).
Remarks: There is 3 levels of selection. 

C. Key Lock / Unlock Keypad
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1. Press and hold MENU key for 2 seconds to lock the key, then LCD screen will display key lock icon(Fig 1). 

2. Only MENU key is activate when Key lock. 

3. Repeat the above operation to unlock, the key lock icon on the LCD screen will disappear.

D. Select the same channel
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Press MENU key once to select channel selection CH menu(Fig 2).  
2. Press UP or DOWN key, select your needed channel.
3. Press PTT key to confirm the channel and return to main screen
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E. Subcode Selection
1. Press MENU key to enter SC setting(Fig 3).

2. Press UP or DOWN KEY to select SUB CODE（00-99）
3. Press PTT key to confirm the sub-code and return to main screen
Remarks: If SUB CODE is 00, LCD display will not shown 00.

F. Make a Call
Press CALL key once to make a calling tone to your friend, one call per minute.
G. Transmitting Message

Press and hold PTT key to talk (with MIC) to other user, “[image: image11.jpg](=



”shows on the LCD screen  to indicate transmission status.
H. To Receive a Call
Release PTT or CALL key and wait for signal. [image: image12.jpg]


 shows on the LCD screen to indicate radio is in receiving mode.

I. Talk Over Earphone

Simply plug the earphone into the Earphone Jack, press PTT key of the earphone and speak.
Function set-up

A VOX function

VOX is the voice activating transmission function. You

can talk and communicate with the other user without

holding the PTT button down 
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1. Press the MENU key to enter into the Vo setting

2. Press UP/DOWN key to set the sensitivity level (Fig5-7) or OF (Fig. 8) 
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    Larger number means a higher VOX mic. sensitivity and vice versa         Fig 5          
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3. Press the PTT key to confirm VOX mode and back to the main screen

Remark： 

- Default setting is off

  - the VOX icon shows on the screen upon VOX is truned on
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 Automatic channel scan and Auto squelch (SQ)
1. Press MENU key to enter into Scan setting.(Fig 9)
2. Press UP/DOWN key to start the channel scan, the Scan icon and changing scanned channels will be show on the screen（Fig.10)
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 The channel number will change. once the signal is detected, channel scanning stops after press PTT key
Activate / Close the Monitoring Function
1. Can activate the monitoring function under the weak signal so as to receive all the signals in this channel 
2. Press MENU key to enter menu M setting(Fig 11)
3. Press UP/DOWN key to activate the monitoring function and return to the main screen automatically 

Activate the monitoring function: Low anti-interference capability, longer distance can be achieved 
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Close the Monitoring Function: High anti-interference capability, shorter distance can be achieved
4. Press PTT key to confirm the setting and return to main screen
Remark: 
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- Under the monitoring status, press the MENU key, it will close the monitoring function automatically
C. Selecting the Call Tone
1. Press MENU key to enter menu CL setting(Fig 12).
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Press UP or DOWN key to select Call Tone(01-05), Call tone demonstration will be heard in each selection
3. Press PTT key to confirm the setting and return to main screen 

Remarks: The default setting of Call Tone is 01
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Selecting the Key Beep
Activate / Inactive the key beep according to your own preference 

1.  Press MENU key to enter menu KB setting
2.  Press UP or DOWN key to set key beep to be On(Fig 13)or OF(Fig 14)
3.  Press PTT key to confirm the key beep setting and return to the main screen
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Remarks: The default setting of key beep is ON
C. Selecting the Roger Beep
When the another party has activated the Roger Beep Function, the user can hear an ending tone (roger beep) when ending the talk.
1. Press MENU key to enter menu R setting
2. Press UP or DOWN key to set the Roger Beep to be On(Fig 15)or OF(Fig 16)
3.  Press PTT key to confirm and return to the main screen
Remarks: The default setting of roger beep is ON

H.  High Low Output Power Selection
1.  Press MENU key to enter power selection menu HP setting
2.  Press UP or DOWN key to set power to be On(Fig 17)or OF(Fig 18)
OF: Higher transmission power, longer distance, but high battery consumption
On: Low transmission power, shorter distance, but low battery consumption 
3.  Press PTT key to confirm and return to the main screen
Remarks: The default setting is (ON)

LCD Backlight

LCD Backlight would be on for 5 seconds once any key is pressed.  
Return to the main screen automatically
When the menu is pressed, if there is no operation in 10 seconds, it will return to the main screen automatically.
Setting Memory
All setting set before the radio is off are memorized and will automatically resume to it when turning on the radio again, The unit will return to the previous setting when it is activated again.

TECHNICAL SPECIFICATIONS
Description




Specifications　　　　　　　　　　　　　　　　　　　　　

Power Output ERIP


≦ 500mW

Operating Frequency


PMR 446.00625 ~ 446.09375MHz 

Channels




8

Sub-code


        99

Modulation                  
FM

Communication Range

Un-obstructed conditions: Up to 3 km　

Power Source



AAA * 3  

Battery Life             6 hours (This time is divided into 90% Standby, 5% Transmission, 5% Reception)
Fully Charging Time          < 12 hours
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