
WT-549 USER MANUAL

BUTTONS AND CONTROLS

[image: image22.jpg]ot

Fig.18





Congratulations

You have just purchased a qualified 2 way radio. 
Please read this manual carefully before use for correct operation.

You should also handle this manual with care for future reference.

Main Screen (Fig.1)

[image: image1.png]ANTENNA———

CALL KEY
PTT KEY— LCD DISPLAY
“+HKEY —”KEY

POWER KEY MENU KEY
MICROPHONE —

SPEAKER



1. Operation Mode Indicator

2. Channel Number Display
3. Key Lock Indicator

4. Battery Icon

5. Channel Scan Indicator

6. Transmission Indictor
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7. Reception Mode
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BATTERY INSTALLATION
Switch off the radio and open the battery door.

Install 3 AAA alkaline batteries (not included) according to the anode-cathode signs as shown.

Replace the battery door.
Note: To reduce the risk of fire or injury to persons while using battery(ies), read and follow these instructions.

- Use only the type and size battery(ies) specified in the operation instructions.

- Do not dispose of the battery(ies) in fire.

- Do not open or mutilate the battery(ies). 

- Exercise care in handling battery(ies) in order no to short out the battery(ies) with conducting materials such as rings, bracelets, and keys. 

- All batteries should be replaced at the same time. 

- Take out battery if long time no use.

- Discard “dead” battery(ies).

Quick Guide

A. Start to Operate

Power On / Off
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1. Press and hold “Power Key   ” key for 2 seconds to turn on the unit.

2. A “Bi” sound indicates the unit is ready for use and the LCD display will show all icons.

3. After 1 second, the unit will go to standby mode. (Fig.2) 
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4. Press and hold “Power Key   ” key for 2 seconds again to power off the unit. A “Bi” sound will also be heard, indicating the radio is going to be switched off.
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Lock / Unlock Key

1. Press and hold “MENU” key for 2 seconds to lock the key. (Fig. 3)

2. Only PTT & CALL buttons can be activated during key locked operation.
2. To unlock the key, press and hold “MENU” button for 2 seconds.

B. “Walkie Talkie” Operation
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Select the same channel as that of your friend’s. e.g. CH=01
1. Press MENU button one time to enter Fig.4.

2. Press + or – button to change the channel. 
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3. Press    button to confirm the setting and return the main screen.

To Make a Call

Press CALL button once to make a call ring tone,  “TX” shows. (Fig.5) 
Transmitting Signal

Press and hold PTT button and speak into the microphone. “TX” shows.(Fig.5)
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To Receive a Call

Release CALL or PTT key and wait for signal. “RX” means the radio is in receiving status. You can hear the call tone or the voice from other user.(Fig.6) 

Adjust Volume Level

1. Press + or – button to enter Fig.7. 
2. You will see the same display as Fig. 8 after a half second.

3. Press + or – button to adjust the volume level from 01 to 07
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4. Press    key to confirm the setting and return the main screen.
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Function Setup

Walkie Talkie Setup Procedure
You may simply set up the function by referring the table below:
	Function
	Channel Selection
	Auto Channel
Scan
	Monitor
	Call Tone
	Key Tone
	Roger Beep

	Application

	
	Select the channel for communication
	Scan the channel automatically to identify the occupied channel
	Received all signal in the same channel during weak transmission
	Call your partner by sending a call tone
	Activate/inactive the key beep according to your own preference 
	Let your partner know the conversation is ended.

	Operation

	Number of   time to press MENU key for entering the selection menu
	1
	2
	3
	4
	5
	6

	Selection Key
	+ / -
	NOT appliable
	+ / -
	+ / -
	+ / -
	+ / -

	Confirmation Key
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	LCD Display
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Press +/- to select the channel.

	
Press   to start channel scanning.

Start channel scanning from the present channel.


Channel scanning stops until the signals is detected.
	
Press +/- to activate / inactive the monitor function.
	
Press +/- to select the call tone.
	
Press +/- to activate / inactive the key beep function.
	
Press +/- to activate / inactive the roger beep function.

	Remark:

	
	Two radios have to be in the same channel in order to communicate each other.
	If no signal detected within 10 seconds or any keys pressed, the channel scanning function will be interrupted. It will then maintain previous channel.
	The monitor function will automatically turn off by press any key except PTT and CALL keys.

Loud noise results if use monitor function under good transmission.
	The default setting of Call Tone is 01.
	The default setting of Key Beep is ON.
	The default setting of Roger Beep is ON. 


B. Other Functions


Auto Squelch (SQ) 

Auto Squelch Control eliminates unwanted interference during communication.
Low Battery Indication

When the battery level becomes low, the battery icon flashes twice per second. When the battery is too low, the unit will be off automatically. 
Attention:

* If the radio is ON while charging, the LCD screen as Fig.9.

* If the radio is OFF while charging, the LCD screen as Fig.10.

* While charging all functions is available for use except PTT key.

TECHNICAL SPECIFICATIONS

Description                   Specifications

Power Output                  ≤ 0.5W   

Operating Frequency          462.5625 ~ 462.7250MHz
Channel                       8
Modulation                    FM

Talk Range                    Up to 3km in clear unobstructed conditions

Power Source                 3 AAA Alkaline Batteries 

Battery Life                   15 hours 

(5% Transmitting, 5% Reception, 90% Standby)

Transmit-Receive Frequencies 

	Channel
	Frequency(MHz)
	Channel
	Frequency(MHz)
	Channel
	Frequency(MHz)

	1
	446.00625
	4
	446.04375
	7
	446.08125

	2
	446.01875
	5
	446.05625
	8
	446.09375

	3
	446.03125
	6
	446.06875
	
	


Trouble Shooting

	Problem
	Solution

	No Power
	- Reposition or replace batteries

	Message Not Transmitted
	- Make sure the PTT button is completely pressed as you transmit.

- Reposition or replace batteries 

	Message Not Received
	- Confirm radios have the same channel settings.

- Make sure PTT is not inadvertently being pressed.

- Obstructions operating indoors or in vehicles 

  may interfere with communication.

- Change your location. 

- Check to make sure volume is loud enough to be 

  heard.

- Reposition or replace batteries

	Hearing Other 
Conversation or Noise on a Channel
	- Shared channel may be in use, try another.

	Limited Talk Range
	- Steel/concrete structures to each other, heavy

foliage will decrease communication range, check

for clear line of sight to improve transmission.

- Wearing radio close to body such as in a pocket

  or on a belt will decrease range, change location 

  of radio.

	Heavy Static or 
Interference
	- Radio are too close to each other. Radio must be 

  at least 15 feet apart, increase your distance.

- Radio are too far apart. Obstacles interfere with 

  transmission.

- Talk range is up to 3 km in clear and unobstructed 
conditions.


Caution:

- Please use only supplied accessories or optional accessories produce by our company or it might cause defect or damage to the unit. 

- Please refer our distributor for optional accessories produce by our company.

- To reduce the risk of electric shock, do not expose this appliance to rain or moisture.

- Do not hold the antenna while the radio is in use, or transmissions quality 
affected.

- Your walkie talkie set has been fully adjusted prior to shipment from the 
factory. Never open your communicator’ s case or adjust the settings inside 
the communicator.

- Never change or replace anything in your communicator except the battery.

- To clean your radio, use a soft cloth dampened with water. Do not use 
corrosive chemical solvent, they may harm the body of the unit and leak inside, causing permanent damage.
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