WT-555 (PMR) USER MANUAL
You have just purchased a qualified 2 Way Radio. Please read this operation instruction carefully before use and keep it. 
BUTTON AND CONTROLS
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BATTERY INSTALLATION
1. Switch off the radio and open the battery door.
2. Install 3 AAA alkaline batteries (not included) according to the anode-cathode signs as shown.

3. Replace the battery door.
Note: To reduce the risk of fire or injury to persons while using battery(ies), read and follow these instructions.

- Use only the type and size battery(ies) specified in the operation instructions.

- Do not dispose of the battery(ies) in fire.
- Do not open or mutilate the battery(ies). 

- Exercise care in handling battery(ies) in order no to short out the battery(ies) with conducting materials such as rings, bracelets, and keys. 
- All batteries should be replaced at the same time. 
- Take out battery if long time no use.
- Discard “dead” battery(ies).

OPERATION

Power On/Off
1. Press and hold   key for 3 seconds until “Di” sound to indicate the unit is power on. LCD will show the current channel.
2. Repeat the above operation to power off the unit.

Adjust the volume
1. Press   key once, the current volume level will show on the LCD screen.

2. Press ▲/▼ key to increase or decrease volume level from L1 to L4(1-4 level). 
3. When volume setting reaches the maximum or minimum level, alert beep tones will be heard.
Channel Selection

Two radios have to be in the same channel in order to communicate each other. 

Select desired channel by pressing and releasing ▲/▼ key. Current channel will be shown on LCD.
To make a Call
1. Press CALL key once to call other parties. 

2. There are short calling melodies indicate the starting and ending of transmitting cal tone.

Transmitting Signal
Press and hold PTT key and speak into the microphone.

Receiving Signal
Release PTT or CALL key and wait for signal.
Low Battery Indicator
When the battery level becomes low, “Bi Bi” alert will be heard every 2 seconds and “LL” will be shown on LCD. The radio will be off automatically after 3 minutes except to replace new batteries.
TECHNICAL SPECIFICATIONS

Description



  Specifications                                      

Power Output


  <500mW 

Operating Frequency

  462.5625 ~ 462.725MHz

Channels


      22
Modulation



  FM

Communication Range
  Un-obstructed conditions: Up to 3 km 

Power Source             3 AAA Alkaline battery  

Battery Life
              > 26 hours (5% Transmitting, 5% Reception, 90% Standby)
PMR446 Transmit-Receive Frequencies(MHz)
	Channel
	Frequency(MHz)
	Channel
	Frequency(MHz)
	Channel
	Frequency(MHz)

	1
	462.5625 
	9
	467.5875 
	17
	462.6000 

	2
	462.5875 
	10
	467.6125 
	18
	462.6250 

	3
	462.6125 
	11
	467.6375 
	19
	462.6500 

	4
	462.6375 
	12
	467.6625 
	20
	462.6750 

	5
	462.6625 
	13
	467.6875 
	21
	462.7000 

	6
	462.6875 
	14
	467.7125 
	22
	462.7250 

	7
	462.7125 
	15
	462.5500 
	
	

	8
	467.5625 
	16
	462.5750 
	
	


TROUBLE SHOOTING
	Problem
	Solution

	No power
	- Reposition or replace batteries

	Message not transmitted
	- Make sure the PTT is completely pressed as
 you transmit.

- Reposition or replace batteries 

	Message not received
	- Confirm radios have the same channel setting.

- Make sure PTT is not inadvertently being pressed.

- Obstructions operating indoors or in vehicles may interfere
 with communication.

- Change your location. 

- Check to make sure volume is loud enough to be heard.
- Reposition or replace batteries

	Hearing other conversation or noise on a channel
	- Shared channel may be in use, try another.

	Limited talk range
	- Steel/concrete structures between each other, heavy foliage
will decrease communication range, check for clear line of
sight to improve transmission.
- Wearing radio close to body such as in a pocket or on a belt
 will decrease range, change location of radio.

	Heavy static or interference
	- Radios are too close to each other. Radio must be at least 

 15 feet apart, increase your distance.

- Radios are too far apart. Obstacles interfere with transmission.

- Talk range is up to 3 km in clear and unobstructed conditions.


Caution:

- Do not expose this appliance to rain or moisture.

- Do not hold the antenna while the radio is in use, or transmissions quality affected.

- Never change or replace anything in your communicator except the battery.

- No naked flame sources, such as lighted candles, should be placed on the apparatus.

- To clean your radio, use a soft cloth dampened with water.
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