
WT-557 USER MANUAL
Congratulations
You have just purchased a qualified 2 Way Radio. Please read this operation instruction carefully before use. If you follow up the operation instructions and cautions of this instruction manual, it will surely bring you the happy radio communication experience. Please keep this operation instruction with care for future reference.
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Safety Precautions
Please read the following precautions before using the interphone:

General rules:

◇ Please keep the distance between the antenna and head & body to be about 2.5 centimeters.
◇ Please use the special accessories for this unit or the optional accessories produced by the company, otherwise it may possibly cause trouble or damage to the interphone. For the optional accessories produced by the company, you can inquiry with our distributor.
◇ Please note that this product is using the common communication channel, if has other users to set it in the same channel, it has the opportunity to receive the communication signal transmitted by this product, you can also receive the signal from the other users.
◇ Do not expose this unit to rain or any type of moisture.
◇ This interphone is not a toy, please be careful not to be used by the children. Should ensure this interphone to be used within the valid communication range.

· Please don’t try to change this interphone.

Environmental conditions

◇ Avoid using under the improper environment, such as: dirt, moisture and extreme high/low temp. environment. Operation under the environment of below humidity 85% can reach better efficiency.
◇ Close this interphone in the places sticking the notice that the interphone or mobile phone is prohibited for using. 
◇ Avoid extruding LCD with heavy force, if so, the LCD will be damaged. 

· Please don’t use this interphone in the places with high humidity and much dirt.
Battery

◇ Avoid any conductor such as: jewelry, key or metal necklace to touch the end part of the battery, if so, the conductor can cause short circuit and result in the battery is too hot or exploding.
· If your product uses rechargeable battery(ies), charge the battery(ies) only in accordance with the instructions and limitation specified in the User Manual.
Electromagnetic interference / Compatibility
◇ Can not change the transmitting frequency, expand the transmitting power freely(including to fix transmitting frequency power amplifier additionally), and can not connect the antenna outside or change to use the other transmitting antenna freely.
◇ Can not create harmful interference to all kinds of legal radio business when using. Once the harmful interference is found, it must be stopped for using immediately, and it can not be used continuously until the interference is eliminated by adopting measures. 
◇ When using the public interphone, its communication quality will not be protected by the radio management body, and should bear the interference created by the other normal working radio business possibly.
◇Prohibit to connect with the public telephone network, public mobile communication network and other communication network.
◇ All the functions of WT-557 have been preset before saling, except for changing batteries, can not open the housing to change the electric circuit and components.
· Almost each kind of electronic device will be effected by the Electromagnetic interference easily. In order to avoid interference, don’t approach the electronic device when using WT-557.
Buttons and Controls
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Main Screen
1. VOX
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2. Scan
3. roger beep
4. Transmitting status (TX) or receiving status(RX)

5. Channel 
6. Key Lock
7. Subcode
8. Battery Level Indicator
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   -- Low Battery:      Blinks, need battery change or recharging.
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   -- Charging:      battery icon will be displayed but not blinks.
Remarks:

When you turn on the unit, LCD display will show all icons. After 1 second, the unit will go to standby mode. 

Other Features of Various Symbols Shown on the LCD.
	Symbol
	Major feature

	[image: image2.jpg]



	Channel Selection
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	Subcode Selection
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	Auto-scan of Channel
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	Monitor Function
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	Call Tone Selection
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	Key Beep
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	Roger Beep
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	Power Selection
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	VOX Function


Battery Installation
1. Switch off the radio and remove the belt clip.

2. Open the battery compartment door.
3. Insert batteries according to the anode-cathode signs shown inside battery compartment
4. Close the battery compartment door.
Note:
1. Don’t mix new and old, different styles, alkaline and rechargeable and different capacity battery.
2. There is a danger of explosion if battery is incorrectly replaced. Replaced only with the same or equivalent type.
3. Attention should be drawn to the environmental aspects of battery disposal.
4. To avoid battery leakage, remove batteries if it is not used for a long time.
5. When the batteries are damaged, please disregard and dispose them with care. Do not dispose of the batteries to heat source to avoid explosion.
Recharging Function
Low Battery Alert
When the battery level becomes low, the battery icon blinks twice in every second. When the battery is too low, the unit will power off automatically. Please change the batteries. If you use NIMH rechargeable, please used supplied charging adaptor for charging. Please do not charge it over 8 hours or the unit may not function properly.
Use charging adaptor for charging: 
   Connect the adaptor side into socket and connect the charging jack hole at the top of the unit, you can charge two units at the same time.Battery icon appears on the LCD when the unit is in charging. Battery icon disappears when the unit is fully charged after 8 hours.
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     Charging when unit is turned off       Charging when unit is turned on
Note:

☆ Please fully charge the rechargeable batteries before first time usage.
☆ This is a danger of explosion or product damage if Alkaline batteries is placed inside battery compartment for charging.
☆ Please use only the supplied rechargeable batteries, AC/DC adaptors for charging, otherwise may damage the unit or may cause explosion.

☆ When the unit is power on and charging, PTT and CALL key is not activate.

Quick Start
A． Power On / Off
[image: image23.jpg]


1.  Power On: Press and hold    key for 2 seconds to power on the radio; Meanwhile there is a “Beep” sound to indicate the unit is power on.
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2.  Power Off: Press again    for 2 seconds during standby operation to turn off the radio, A “Bi” sound will also be heard, indicating the radio is going to be switched off.
Remarks: When the walkie talkie is connected with the power supply, it will power on automatically.
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Key Lock / Unlock Keypad
1. [image: image26.jpg]


Press and hold MENU key for 2 seconds to lock the key, then LCD screen will display key lock icon(Fig 1). 

2. Only PTT & CALL buttons can be activated during key locked operation. 

3. Repeat the above operation to unlock, the key lock icon on the LCD screen will disappear.
C. Select the same channel
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Press MENU key once to select channel selection CH menu(Fig 2). 
2. Press UP or DOWN key, select your needed channel. 
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Press    key to confirm the channel and return to main screen
D. Subcode Selection
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Press MENU key to enter SC setting(Fig 3).
2. Press UP or DOWN KEY to select SUB CODE（00-38）.
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Press    key to confirm the sub-code and return to main screen.

Remarks: If SUB CODE is 00, LCD display will not shown 00.
E. Make a Call 
Press CALL key once to make a calling tone to your friend.

F. Transmitting Message
Press and hold PTT key to talk to other user, “[image: image11.jpg](=



”shows on the LCD screen  to indicate transmission status.
G. To Receive a Call
Release PTT or CALL key and wait for signal. [image: image12.jpg]


 shows on the LCD screen to indicate radio is in receiving mode.
H. Talk Over Earphone

Simply plug the earphone into the Earphone Jack, press PTT key of the earphone and speak.
Function Setting
A. [image: image33.jpg]


Volume Level Adjustment
1. Press UP or DOWN key to select the volume level from 01 to 07(Fig 4).
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Press    key to confirm the volume level setting and return to main screen.
B. Activate / Close the (VOX)
User can can talk and communicate with each other without pressing and holding the PTT button. There is 3 levels of selection. 
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Press MENU key to enter menu Vo setting.

2. [image: image37.jpg]


Press UP or DOWN key to set sensitivity level(Fig 5--7) or OF(Fig 8).
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The higher sensitivity level, higher VOX/ MIC sensitivity.

· The Lower sensitivity level, Lower VOX/MIC sensitivity.
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3.  Press    key to confirm the setting and return to main screen.
Remarks:

-- The default setting of VOX function is OFF.

-- When setting VOX ON, “VOX” shown on the LCD.


C. Activate / Close the Auto-scan of Channel
1. Press MENU key to enter menu Scan setting(Fig 9).
2. Press POWER key to start scanning, LCD will display “Scan”icon and channel number of changed scanning(Fig 10). 
3. Channel scanning stops once the signal is detected.

D. Activate / Close the Monitoring Function

Can activate the monitoring function under the weak signal so as to receive all the signals in this channel. 
2. Press MENU key to enter menu M setting(Fig 11).
3. Press POWER key to activate the monitoring function and return to the main screen automatically.
· Activate the monitoring function: Low anti-interference capability, longer distance can be achieved.
· Close the Monitoring Function: High anti-interference capability, shorter distance can be achieved.
Remarks:
-- Under the monitoring status, press the MENU key, it will close the monitoring function automatically.
-- Under the monitoring status, Press PTT key, call key, UP/DOWN key, the monitoring status is unchanged.
E. Selecting the Call Tone 
1. Press MENU key to enter menu CL setting(Fig 12).

2. Press UP or DOWN key to select Call Tone(01-05), Call tone demonstration will be heard in each selection. 
3. Press    key to confirm the setting and return to main screen.
Remarks: The default setting of Call Tone is 01.

F. Selecting the Key Beep
Activate / Inactive the key beep according to your own preference.

1.  Press MENU key to enter menu KB setting.

2.  Press UP or DOWN key to set key beep to be On(Fig 13)or OF(Fig 14).
3.  Press    key to confirm the key beep setting and return to the main screen.

Remarks: The default setting of key beep is ON.

G. Selecting the Roger Beep
When the another party has activated the Roger Beep Function, the user can hear an 
ending tone (roger beep) when ending the talk. 
1. Press MENU key to enter menu R setting.

2. Press UP or DOWN key to set the Roger Beep to be On(Fig 15)or OF(Fig 16).
3. Press   key to confirm and return to the main screen.
Remarks: The default setting of roger beep is OFF
H. High Low Output Power selection
1. Press MENU key to enter power selection menu HP setting.
2. Press UP or DOWN key to set power to be On(Fig 17)or OF(Fig 18).
· OF: Higher transmission power, longer distance, but high battery consumption.

· On: Low transmission power, shorter distance, but low battery consumption.


3. Press POWER key to confirm and return to the standby mode.

Remarks: The default setting is OFF.
I. Activate / Close Torch function
Press [image: image13.jpg]


 key to activate. Release the [image: image14.jpg]


 key to switch off.
Other Functions setting
LCD Backlight
LCD Backlight would be on for 5 seconds once any key is pressed.
Return to the main screen automatically
When the menu is pressed, if there is no operation in 10 seconds, it will return to the main screen automatically.
Setting Memory
All setting set before the radio is off are memorized and will automatically resume to it when turning on the radio again, The unit will return to the previous setting when it is activated again.
Fast Changing of Channels

Use UP or DOWN key to select the menu or adjust channels, sub-code, volume, etc., it will change the number sequentially if you press the UP or DOWN key for more than 1 second.
TECHNICAL SPECIFICATIONS
　　　　　　　　　　　　　　　　　　　　
Description                Specifications
Power Output                ≦ 500mW
Operating Frequency
        446.00625 ~ 446.09375MHz
Channels                   8
Sub-code                   38
Modulation                  FM　
Communication Range       Un-obstructed conditions: Up to 5 km
Power Source               AAA *  4 
Battery Life             8 hours(This time is divided into 90% Standby, 5% Transmission, 5% Reception)
Fully Charging Time          < 12 hours

Transmit-Receive Frequencies
	Channel
	Frequency(MHz)
	Channel
	Frequency(MHz)
	Channel
	Frequency(MHz)

	1
	446.00625
	4
	446.04375
	7
	446.08125

	2
	446.01875
	5
	446.05625
	8
	446.09375

	3
	446.03125
	6
	446.06875
	
	


CTCSS SUBCODE (HZ)
	Code
	Frequency(Hz)
	Code
	Frequency(Hz)
	Code
	Frequency(Hz)

	1
	67.0
	14
	107.2
	27
	167.9

	2
	71.9
	15
	110.9
	28
	173.8

	3
	74.4
	16
	114.8
	29
	179.9

	4
	77.0
	17
	118.8
	30
	186.2

	5
	79.7
	18
	123.0
	31
	192.8

	6
	82.5
	19
	127.3
	32
	203.5

	7
	85.4
	20
	131.8
	33
	210.7

	8
	88.5
	21
	136.5
	34
	218.1

	9
	91.5
	22
	141.3
	35
	225.7

	10
	94.8
	23
	146.2
	36
	233.6

	11
	97.4
	24
	151.4
	37
	241.8

	12
	100
	25
	156.7
	38
	250.3

	13
	103.5
	26
	162.2
	
	


Communication Environment
1. General communication environment(the following figure 1）
a. Within the communication range, there is no equipment produces the interference signal which power is more than or equal to output power of WT-557, for example high voltage power cable, radio station & etc.
b. Within the communication range and under open area, there is no large-scale buildings with metal act as the block. 
2. Perfect communication environment(the following figure 2）
Based on above 2 general communication environments and under open areas, communication range can be over 5 km when 2 communicators are positioned at horizontal straight sight.

3. Poor communication environment(the following figure 3）
There is solid block between 2 communicators, it is suggested not to communicate under this environment.
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1.General Communication      2.Perfect Communication        3.Poor Communication
Environment                  Environment                   Environment
Caution and safety notice
In order to prevent the hazard from user and other people, it will possibly cause the serious results of serious harm and dead etc by misusing.
If happened the following abnormal conditions when using or recharging, please take out the batteries and plug out the recharging power source immediately and stop using. It will happen the events of short circuit, heating, burning or electric shock of poor insulation etc if using continuously. Please consult with your distributor, absolutely not to repair it by yourself.
☆ Smoking, abnormal heating, abnormal smell(burning smell), please don’t use it, and take out the batteries.
☆ If there is other material inside the product, please don’t use it, and take out the batteries and stop working.
☆ If the housing is broken or damaged, please don’t use it, and take out the batteries and stop working.
☆ If the battery surface is broken or damaged, peeled etc, or the bobbin of power cord is exposed etc, please don’t use it, and take out the batteries and stop working.
Caution!
☆ Please don’t plug out the power source plug or operate the switch by wet hand, otherwise it will cause electric shock easily.
☆ Please don’t disassemble and change the product, additionally, someone must not disassemble and repair it who is not in charge of repairing, otherwise it will happen the events of short circuit, burning,fault or electric shock etc.
☆ If the specification of the socket and wiring apparatus excesses the load, please don’t use it. If the wiring excesses the specification too much, it will happen the events of heating, burning or electric shock etc.
☆ Please don’t use the broken or damaged power cord or plug as well as power source plug with dirt etc., otherwise it will happen the events of short circuit, heating, burning or electric shock of poor insulation etc.
☆ Please ensure not to use the power source plug until it is plugged into the socket. otherwise it will happen the events of heating, burning or electric shock etc.
☆ Please don’t let this unit approach the container with water, such as: tub, shower and natatorium. If this unit infalled with water, please don’t use it, and please contact the distributor.
☆ Please don’t put it in the unstable places of wobble or leaning etc. Because it will be affected by earthquake or outer force, easily make the product spilled, so cause the dangerous of injury, and make the product failed or damaged.
☆ Please don’t touch the antenna and power source connector when it is thundering. 
Caution:
☆ Please don’t extrude or bend the power cord excessively.
☆ Do not place heavy and lighted objects such as candles, cigarettes on the unit.
☆ They are provided for ventilation and protection against overheating, please don’t block it. Please don’t put it on the objects of table covered with table cloth, carpet, quilt etc.
☆ Please make sure to plug off the power cord and connecting wire when moving this unit, Please don’t let this unit bumped when using it.

☆ Please don’t spray the insecticide or volatility substance onto the housing surface of this unit, otherwise it will easily make the product housing damaged and result in fault, or cause the accidents of electric shock and burning etc.
☆ Use a soft and damp cloth for cleaning. Do not use the solution contained corrosion chemical product for cleaning.
Trouble Shooting
	Problem
	Solution

	No Power
	Reposition or replace batteries.

	Message Not Transmitted
	1. Make sure the PTT button is completely pressed as you 
transmit.
2. Make sure the microphone hole has not been block.
3. Reposition or replace batteries.

	Message Not Received
	1. Confirm radios have the same channel and sub-code setting.
2. Make sure PTT is not inadvertently being pressed.
3. Reposition or replace batteries.
4. Obstructions operating indoors or in vehicles may interfere with communication. Change your location. Check to make sure volume is loud enough to be heard.

	Hearing Other Conversation / Noise from the other walkie talkie or channel
	1. Confirm this channel or sub-code is being used.
2. Try another channel and sub-code.

	Limited Talk Range
	1. Steel/concrete structures between each other, heavy

foliage will decrease communication range, check for 

clear line of sight to improve transmission.
2. Wearing radio close to body such as in a pocket or on a
    belt will decrease range, change location of radio.

	Heavy Static or Interference
	1. Radio are too close to each other. Radio must be at 
   least 2 meters apart, increase your distance.
2. Radio are too far apart. Obstacles interfere with 

   transmission.
3. Talk range is up to 5 km in clear and unobstructed 
   conditions.

	Keyboard is invalid.
	1. The keys are locked, need to unlock the key lock firstly.
2. The keyboard will be frozen temporarily when the radio is transmitting. If you press the PTT suddenly, please release it.
3. Under the VOX condition, it will also make a transmission even if you do not press the PTT, you can close the radio to activate it again.
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