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Congratulations

You have just purchased a quality baby monitor. Please read the instructions thoroughly before using the monitor system and keep it for future reference.

Safety Precautions                                              

When using this unit, basic Safety Precautions should always be followed to reduce the risk of fire, electric shock, or personal injury.

1. Read and understand all instructions.

2. Follow all warnings and instructions marked on this unit or mentioned in this operation 
instruction.

3. Do not use liquid or aerosol cleaners. Use a damp cloth for cleaning.

4. Do not use this unit near water such as bathtub, shower or pool. Immersion of this unit 
in water could cause an electrical shock.

5. Place the unit securely on a stable surface. Serious damage and/or injury may result if 
the unit falls.

6. Do not cover slots and openings on the unit. They are provided for ventilation and 
protection against overheating.

7. Install the unit where no one can step or trip on the cord.

8. Never push any objects through slots in this unit. This may result in the risk of fire or 
electric shock. Never spill any liquid on the unit.

9. To reduce the risk of electric shock, do not disassemble this unit. Take the unit to 
authorized service center or qualified technician when service or repair work is required. Opening or removing covers may expose you to dangerous voltages or other risks. Incorrect reassembly can cause electric shock when the unit is subsequently used.

10. Do not expose the unit to extreme temperatures such as areas near a hot radiator or stove or in a hot car.

11. Do not place lighted objects such as candles, cigarettes on the unit.

Caution:

This product cannot replace responsible adult supervision.
· This Baby Monitor is intended as an aid. Do not use it as a medical monitor or a substitute for responsible and proper adult supervision. 

· Make sure the Parents unit and adaptor cable are always out of child's reach. Do not place the Baby Unit inside the baby's crib or playpen!
WARNING: 

To prevent the risk of fire or electrical shock, do not expose this unit to rain or any type of moisture.

Content and Features
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Baby unit :

[image: image6.png]



1.  LCD Display

2.  Microphone

3.  Speaker

4.  Belt Clip

5.  Lock / Unlock key

6.  Battery Compartment

7.  Power and Volume Control

8.  AC / DC Power Supply Sock

9.  PAGE key

10. Music Play and Control 

11. LINK key

Parents unit :
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1. LCD display 

2. Microphone

3. Speaker

4. Belt Clip

5. Lock / Unlock key 

6. Battery Compartment

7. Power and Volume Control

8. AC / DC Power Supply Sock

9.TALK key

10.PAGE key

11.Music Play and Control 
12.LINK Key

Main LCD Screen
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AC Adaptor:

[image: image10.jpg]MG SO0

[[[LLiges NI AS'2 00

0—
32071 O 320NN




The AC Adaptors are low voltage power source that allow you to use your household electricity to run the Baby Monitor.  Connect the AC Adaptors to the AC Adaptor Jack in the Unit.  Both plug into any standard volt electrical outlet in your home.  It is recommended to turn off the units before plug in or unplug the adaptors.

CAUTION: These adaptors were made with a specific design for this product. They cannot be used with any other appliance. Never use a different type of adaptor with this Baby Monitor.
Privacy Protection

Always remember that you are using public airwaves when you use the Wireless 2.4GHz Digital Baby Monitor. Sound may be broadcasted to other receiving devices. Conversations, even from rooms near the Baby unit, may be broadcast as well.

CAUTION: To protect your privacy, always turn the system off when not in use. It is possible that the Parents unit may be interfered from other devices in the 2.4GHz frequency range. To minimize this potential problem, more than 65000 ID code have been provided for your use. If you experience interference while using one ID code setting, simply select to another ID code. 

Battery Installation
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Please charge the rechargeable batteries before first time usage.

1. Ensure the unit is off. Press the button on the belt clip and rotate it    

clockwise or counterclockwise for 90º.

2. Open the battery compartment door.

3. Insert 3 * AAA batteries into the Baby unit and Parents unit according to the +/- signs shown in the battery compartment, respectively.

4. Replace battery compartment door. Press and rotate the belt clip to its   

normal position.

Battery Tips:

· If the product is not in use for a long time, disconnect both units from the household electrical outlet. And remove the batteries or the exhausted batteries from the units, otherwise battery leakage and corrosion can damage them.
· Dispose the batteries safely. 

· Non-rechargeable battery is not to be recharged.

· Rechargeable batteries are only to be charged under adult supervision.
· Danger of explosion if battery is incorrectly replaced. Replace only with the batteries of the same and equivalent type(TSUEN SHING, BT-101-AC).
Battery Charging
If the battery level becomes almost empty, the units will display the below : 

	Model
	Baby Unit
	Parent Unit

	

	LCD Display version
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	No Alert sound and empty battery
	Emits a alert tone (Di Di) in every 3 seconds


In this case, user needs to recharge the supplied rechargeable batteries or change for new alkaline AAA batteries.

Charging the batteries

The rechargeable batteries to the Baby unit and Parents unit must not be taken out of the units for charging. 

1. Use only the AC adaptors which are included in the package, plug into any nearby standard household electrical outlet.  

2. Once connect them with the units, charging automatically begins. 
3. The charging time for completely charging empty battery takes 8 hours when the unit is turned off. 

Charging and Fully charged Indication:

	
	LCD version

	In charging

(Unit is turned on.)
	[image: image13.png]


[image: image14.png]



               or

The battery icon loops.

	In charging

(Unit is turned off.)
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The battery icon loops.

	Fully charged

(Unit is turned on.)
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             or
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The battery icon is full and stops looping.

	Fully charged

(Unit is turned off.)
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The battery icon is full and stops looping.


Note:

· User can also install 3 alkaline AAA batteries instead of the supplied re-chargeable batteries.
· Or directly operated by the supplied adaptors. 
Help protect the environment

Batteries with symbols shown opposite must not be disposed in general domestic waste.
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Instead, take them to a collecting point for old batteries or special waste products(as your local authority for details) or return them to the dealer you bought them from. They will ensure batteries are disposed safely.

Testing Before First Time Usage
A. Test the Baby unit transmission and the Parents unit reception.
1. Place Baby unit and Parents unit in room where you intend to use it. 

2. Set both Baby unit and Parents unit to the corresponding code by pressing the LINK key at the bottom of the units for different ID code to ensure privacy.

There are more than 65000 ID codes user selection. 

3. Then, the LCD displays standby status. 

NOTE: 

For the first time usage, turn on both units, they can automatically scan the 

corresponding code at once without press any key. If reset the corresponding code for 

both units, user has to press the LINK key.   

B. Baby unit emission:

1. Place Baby unit in room where you intend to use it.

2. Push the SENSITIVITY switch to a desired position to turn on the Baby unit 

transmission.

3. As soon as the Baby unit transmits a signal, then:
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Constantly changing display-readouts


  4. The transmitter is standby status when no signal is transmitted.
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C. Parents unit reception:

1. Place Parents unit in room where you intend to use it. 

2. Slide the VOLUME switch to a desired position and the unit is ready for reception.

3. If the unit receives a signal, 
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Constantly changing display-readouts 


4. The receiver is standby status when no signal is received. 
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When you experience interference (buzzing or static, etc.), reset both units to another corresponding code. ( details please refer to P.10 – scan the corresponding code for the units )
IMPORTANT!  Test sound reception before use and whenever location of Baby unit is changed. (Refer to Testing Before First Time Usage)
Note:

* Position the Baby unit at least 1 meter away from the baby so that the microphone can pick up the child's sound.
* Unwrap and fully extend power cord for best transmission if adaptor is used. Plug the adaptor into the nearest standard household electrical outlet.
Operations Procedures

A. Power On / Off

1. Connect the Parents unit with the AC adaptor. Plug it into the nearby standard electrical 
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outlet or insert 3 AAA alkaline batteries.
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2. Turn on      at the right side upward of the unit, a click sound to be heard indicates the unit is turned on.

3. Turn     downward, a click sound indicates the unit is off. 
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B. Volume Adjustment

Rotate      for adjusting the desired volume level.  

1. Turning it upward for increasing volume level;

2. Turning it downward for decreasing volume level.

C. Talk to Baby unit (Only for Parents unit) 

TALK key is located at the left side of the Parents unit. 

1. Press and hold TALK key to talk to the Baby unit.

2. Release TALK key and return to the receiving status.

Remark : When the Parents unit is talking to the Baby unit, the call ring tone can also be 

heard if press PAGE key of Baby unit. 
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D. Music Playing & Select Music 

Music play     key is located at the left side of the unit. User can activate the 

music play and/or select a desired music to lull the baby to sleep. There are six music for 

selecting.

1. Press     key for about 3 seconds to activate the Music Playing function, and Music 01 will be played automatically.

2. Press     key to change music(01-06 or AL), you can hear the demonstration of different music. When you have selected the desired music, do not press     key again. 
Note: Selected music will be shown on the top right corner of the LCD screen for LCD version.

3. Press     key for about 3 seconds again to turn off the music playing function.

Remarks : 
- Baby unit can play music solely when the Parents unit is turned off. But Music play function of Parents unit is not available for use when Baby unit is turned off.  

- When pressing the TALK key of Parents unit to talk to Baby unit, the music will be stopped playing.   

- Music playing is not interrupted by call ring tone. 
- Music playing could be interrupted by out of range alert.

E. Sensitivity Level Adjustment (Only for Baby unit)

SENSITIVITY slide switch      is located in the battery compartment. Adjust different 
detecting sound level sensitivity by switching the SENSITIVITY switch to either Lo 
( normal sensitivity : 1-2 meters) or Hi ( high sensitivity : 2-6 meters) position.

Remarks : The default setting of sensitivity level is Hi.

F. Call Function

Both units can make a call ring tone to call one another. 

1. Press PAGE key at the left side of the Parents unit or Baby unit one time to call another unit. 

2. Three “BiBi” sound will be heard from Baby unit or Parents unit.

3. Each press PAGE key once, you will hear three “Bi Bi” sound. If no press PAGE key 

again, the call ring tone will end.

Remarks: 
- When Baby unit call Parents unit, only the Parents unit can be heard three “Bi BI” sound ( with power LED of Parents unit flashes RED light for LED indicator version.)

- When Parents unit call Baby unit, only the Baby unit can be heard three “Bi BI” sound (with power LED of Baby unit flashes Red light for LED indicator version.)
G. Low Battery Alert

When the unit is in low power, the details please refer to page 5 “Battery Charging” . 

Remarks: 

-- No low battery alert for Baby unit.

 -- No transmission and receipt while the unit is in low battery.

H. Out of Range Alert (Only for Parents unit )

When the connection between Parents unit and Baby unit is broken , e.g.

- One of the units is turned off during connection ;
- The Baby unit is in low battery; 

- The units are detected out of communication range.

The units will display the below :

	Parents Unit
	
with “Di Di Di” alart sound will be heard in every 1 second

	Baby Unit
	



For Blue Angel version, when only turn on the Parents unit, out of range alert sound 

should be heard within 30 second. 

Note: Under out of range alert mode, the TALK, PAGE and music play key is not available 

for use. 
I. Key Lock / Unlock 
1. Turn the right-hand key lock side switch               to LOCK position of unit to lock key. The TALK key, PAGE key and MUSIC key are not available for use.

2. Turn the same switch             to UNLOCK position to unlock all the keys.

J. Belt Clip

The Baby unit and Parents unit can both be carried around using the belt clip provided on the rear of each unit.

How to operate 2 way communication between Parents unit and Baby 

unit

The Baby Phone yields high privacy and almost zero-interference to end users. There are 

more than 65000 ID code for user selection with the LINK key positioned at the bottom of 

the units. 
NOTE: 

Only scan the corresponding code for both units, they are able to connect to one 

another. 
Operating and Setup

A. Scan the Corresponding Code

1. Turn on both units. The Baby unit will emit a random ID code to Parents unit 

   automatically without pressing any key. 

2. Once scanned the corresponding code, the units are ready for use. 
The code is recorded even thought you turn off the units or recharge the batteries. Or 

else the unit is not for use.
B. LINK key

LINK key is located at the bottom of the Parents unit and Baby unit. It is used for 

eliminating the corresponding code recorded in the unit and reset a new corresponding 
code for the Parents unit and Baby unit. The Parents unit / Baby unit can connect with 
another Baby unit / Parents unit with the LINK key to scan a new corresponding code for 
them.

1. Ensure both units are turned ON. Press the LINK key of the units with a spiky and 
thin object (such as toothpick).

2. Both units begin to scan corresponding code

	
	Parent unit &Baby unit

	Scanning the corresponding code automatically
	


	Scanned the corresponding code successfully
	
                 OR

normal status    constantly changing display-readouts  
with a “Di” sound


	Scanned the corresponding code unsuccessfully
	



Remarks: If operated by the supplied adaptor, please first plug in the adaptor, then 

power on the unit. And then scan the corresponding code with the LINK key if need.   

C. 2-Way Communication

Usually, the detected sound is transmitted from the Baby unit to Parents unit. But Parents unit can talk to Baby unit with its TALK key. 

1. Press and hold TALK key of Parents unit and talk to the Baby unit.

2. Release the TALK key, the Parents unit is in receiving status and wait for signal from 
Baby unit.

Remarks: 

When pressing TALK key, the Parents unit does not receive any sound from Baby unit.

D. Music Control

After activating Music Play function of both units, as long as one of them adjusts music play or changes music(01-06 or AL), the setting for this function of the other unit will change accordingly.

Trouble shooting 

	Problems
	Solutions

	1. No power
	- Unit is turned off. 
- Check if the batteries are installed properly. 
- Make sure the adaptor is connected to the Unit properly if using the adaptor instead of batteries.
- The Unit may be in low battery status, change new batteries.

	2. Message not 

transmitted.



	- Sound sensitivity level of Baby unit is too low, turn the sound sensitivity switch to “HI” position.
- Units are out of range or lost connection. Ensure the distance between the units within communication range. 
Note: Communication range varies depending on surrounding 
conditions such as physical obstructions, interference.

- Make sure the TALK key of Parents unit is not pressed.
- Make sure the unit is unlocked. 

- Ensure both units have already scanned the corresponding  
code.

	3. No sound signal
	- Volume level on Parents unit is set too low. Adjust it to higher volume.
- Sound sensitivity level of Baby unit is too low, Turn the  

 Sound Sensitivity switch to “HI” positions. 
- Units are out of range. Ensure the distance between the units within communication range.
- Make sure the TALK key of Parents unit is not pressed.
- Make sure the unit is not locked key. 

- Ensure both units have already scanned the corresponding  
code.

	4. Received 

Conversation or 

sound from neighbors.

	- Signal interference due to other nursery monitor on the same ID Code or cordless phone used.

- Change both units to another ID code by pressing LINK key.

	5. Hearing static or rustle from Parent unit.
	- The both units are positioned too close to each other. Keep away two units at about 1m.

- The volume is set too high. Lower the volume at the Parent unit.
- Reposition or replace batteries.

	6. Power LED rapidly flashes green light and can not receive or transmit 
	- The power is too low. Change new batteries or operated by the supplied adaptor.  


Technical Specifications
Power Supply Voltage: 

Parents unit : 3 AAA batteries or rechargeable batteries & 

Adaptor: AC 100V – 240V- DC 5.5V,500mA
Baby unit   : 3 AAA batteries or rechargeable batteries & 
Adaptor: AC100-240V, DC 5.5V, 500mA
Operation Frequency : 2.4015GHz～2.4525GHz

Operating Range:  up to 300m in ideal conditions

Mic Sensitivity : 1 to 2 meter
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Out of range alarm icon





Selected Music: 01-06 or AL


01-06 : Music 01- Music 06 . The selected song will be playing repeatedly.


AL : Play All music – Music is looped from 01 to 06 repeatedly.





Battery icon:


 �  Full battery level


� Low battery level, reminds you to change the batteries.


� Empty and flashing, batteries change is a must.





“Baby sleeping” icon : (no signal and energy saving mode)





“Baby calling” icon : constantly changing display





button





90º





Flashing





Flashing





Flashing





Flashing





still flashing
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