
BM-166 Baby Phone User Manual
Congratulations

You have just purchased a quality baby monitor. Please read the instructions thoroughly before using the monitor system and keep it for future reference.
Content and Features
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1. Soft Antenna                               
2. Channel Switch                                7. AC/DC Power Supply Socket           
3. Sensitivity Control                             8. Battery Compartment          
4. Mic                                                                     

5. Power Indicator                          
6. Power Control
PARENTS UNIT
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1. Soft Antenna                        8. AC/DC Power Supply Socket 

2. Channel Switch                      9. Belt Clip
3. Power Indicator                      10. Wall Mount Hole
4. Sound Lights                        11. Battery Compartment
5. Speaker                           
6. Volume Control                           
7. Power ON/OFF                    
AC Adaptor:

The AC Adaptors are low voltage power source that allow you to use your household electricity to run the Baby Monitor.  Connect the AC Adaptors to the AC Adaptor Jack in the Parents and Baby Unit.  Both plug into any standard volt electrical outlet in your home.  It is recommended to turn off the units before plug in or unplug the adaptors. The mains plug is used as disconnect device, the disconnect device shall remain readily operable.
CAUTION: These adaptors were made with a specific design for this product.  They cannot be used with any other appliance.  Never use a different type of adaptor with this Baby Monitor. 
Important!
- This Baby Monitor is intended as an aid.  Do not use it as a medical monitor or a 
substitute for responsible and proper adult supervision.

- Make sure the Baby Unit and adaptor cable are always out of child's reach. Do not place 
the Baby Unit inside the baby's crib or playpen!

- The antenna on the Parents and Baby Units are fixed, do not try to extend them. Never 
attempt to modify the product.

Color Index of Power Indicator

	 Color of   

       Power Indicator   

Power      

Sources
	Red
	Green

	AC Adaptor Operated

(Baby unit & Parent Unit are On) & stand by
	
	flashing

	AC Adaptor Operated (Units are Off)
	No light

	Battery Operated (Low Battery Level)
	flashing
	

	Stand by (Baby unit & Parent Unit are On)
	
	flashing

	sound received (Baby unit & Parent Unit)
	
	stable


Battery Installation (not included)
1. Locate the battery compartment door on the back of the Parents and Baby Units.

2. Open the battery compartment door.

3. Insert 3 pieces of AAA batteries into the Parents Unit and Baby Unit according to the +/- signs shown in the battery compartment, respectively.
4. Replace battery compartment doors.

Battery Tips:

- If the product is not in use for a long time, disconnect both units from the household electrical outlet. And remove the batteries or the exhausted batteries from the units, otherwise battery leakage and corrosion can damage them.

- Dispose the batteries safely.

- Non-rechargeable battery is not to be recharged

- Rechargeable batteries are only to be used & charged in parent unit under adult supervision.

CAUTION: 
- The batteries shall not be exposed to excessive heat such as sunshine, fire or the like.

- Danger of explosion if battery is incorrectly replaced. Dispose of used batteries according to the instructions. Replace only with the same or equivalent type.
Battery Charging (For parent unit only)
1. Use only the AC adaptors which are included in the package, Plug into any nearby 
standard household electrical outlet.

2. Once connect them with the unit, charging automatically begins. 
3. It takes 8 hours to charge the re-chargeable batteries full at the first time.

4. Please unplug the AC adaptors from electrical outlet or remove the unit from the 
charger stand after completed charging.
Note:

- User can also install 3 alkaline AAA batteries instead of the supplied re-chargeable batteries.

- Or directly operated by the supplied adaptors.

- The power indicator will turn off when the power is out or in low battery. In this case, user needs to re-charge the supplied re-chargeable batteries or change for new alkaline AAA batteries.
Testing Before First Time Usage
IMPORTANT!  Test sound reception before use and whenever location of transmitter is  changed. (Refer to Testing Before First Time Usage) 
Test the Baby Unit transmission and the Parents Unit reception.

1. Power on both units by press Power key at the right side of the units. 

2.
Set both Parents and Baby Units to the same channel (1 or 2) by switching the channel switch. 
3.
 Adjust the appropriate volume level by press VLO+ / VLO- key at the right side of unit.(To adjust volume, please see the “Function Setup)
NOTE:

It is important that with both units the switch setting are the same because if this is not the 

case the baby unit and parents unit will not be able to connect to one another.

4. Place Baby Unit and Parents Unit in room where you intend to use it. 
5. Push the SENSITIVITY switch on the Baby unit to a desired position. 

6.
Red light of sound level indicator on the Parents Unit lights when sound is received:

- One or two dots light for shallow sound received.

- Three or more dots light for louder sound received.
Note:
- Position the Baby Unit at least 1 meter away from the baby so that the microphone can pick up the baby’s sound.

- The Baby Unit will go to a stand-by mode for power saving when it doesn’t detect sound from the surrounding area.

- Unwrap and fully extend power cord for best transmission if adaptor is used. Plug the adaptor into the nearest standard household electrical outlet.

Function Setup

A. Power On/Off
For parent unit:

1. Press and hold the Power key at the right side of both units for 3 seconds until Bi sound to be heard. The power indicator LED flashes green lights indicating the unit is in full battery conditions. (After install battery or connect to adaptor, units will be powered on automatically)
2. Press and hold the Power key for 4 seconds until a Bi sound to be heard and power indicator LED is off indicating the unit is powered off.
For baby unit:

1. Press and hold the Power key at the right side of both units for 3 seconds until power indicator LED flashes green lights indicating the unit is in full battery conditions. (After install battery or connect to adaptor, units will be powered on automatically)

2. Press and hold the Power key for 4 seconds until power indicator LED is off indicating the unit is powered off.
B. Volume Adjustment

1. Press VLO+/VLO- key to adjust the volume level from 1 to 3. Volume level demonstration will be heard in each selection when the unit is receiving.
2. When adjusting up to volume level max.03 or min 01, “Du di“sound will be heard. 
C. Channel Selection

Select the Channel (CHANNEL 1 or CHANNEL 2) by left side channel switch.
D. Sensitivity Level Adjustment (Only for Baby Unit）
Adjust different detecting sound level sensitivity by switching the SENSITIVITY switch to to either NORM (normal sensitivity: 1-2 meters) or HIGH (High sensitivity: 2-6 meters) position.

E. One Way Communication

The detected sound is transmitted from the Baby unit to Parents unit. The Baby unit couldn’t receive signal from Parents unit.

F. Low Battery Alert

When the unit is in low power, the LED power indicator lights red. The Parents unit also emits alert tone (Bi, Bi) in every 19 seconds. In this case, user needs to change for new AAA batteries or powered by adaptor..
Note: No low battery alert for Baby unit.
Trouble shooting
	Problems
	Solutions

	1. No power
	- Unit is not turned on. Turn on the units. 

- Check if the batteries are installed properly. 

- Make sure the adaptor is connected to the Baby Unit properly if using the adaptor instead of batteries.

- The Unit may be battery low, change for new batteries.


	2.No power indicator

lights
	- Volume level on Parents Unit is set too low. Adjust it to 

higher volume.

- Sound sensitivity level of Baby Unit is too low, Turn the 

Sound Sensitivity switch on Baby Unit to High position. 

- Units are out of range.  Move Parents Unit closer to Baby Unit

- Ensure both units are in the same channel.

	3. Hearing static or 

Buzzing from Parents Unit
	- Make sure both units are set to the same channel

- Move the Parents Unit closer to the Baby Unit

Note: Communication range varies depending on surrounding conditions such as physical obstructions, interference.

- Reposition or replace batteries.

	4. Conversations or sounds from other homes received

	- Signal interference due to other nursery monitor on the 

same channel or cordless phone used. Change both units to another channel to eliminate source of interference.

	5. High pitched noise
	- The Parents and Baby Units are positioned too close to each 

other. Move Parents Unit away from Baby Unit.

- The volume is set too high. Lower the volume at the 

Parents Unit.


Technical Specifications

Power Supply Voltage:

Baby Unit-3 AAA alkaline batteries & adaptor: AC100-230V DC 5.5V

Parent Unit-3 AAA alkaline (rechargeable) batteries & adaptor: AC100-230V DC 5.5V

Frequency: CH1:434.140MHz

           CH2:434.340MHz

Channel:2 Channels

Operating Range: up to 1300 meters in ideal conditions

Set includes: 1 baby unit, 1 parent unit, 2 adaptors, 1 user manual.
CAUTION


This product cannot replace responsible adult supervision.


To reduce the risk of electric shock, do not expose this appliance to rain or moisture.


When install the baby unit, it should take extra precautions to install the adaptor wire away from the baby.


The product would not perform normally under the high disturbance from the AC mains.
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