
BM-168 User Manual
TABLE OF CONTENTS

Content and Features……………..………………………………………………………………………

Battery Installation……………………………..…………………………………………………………

Testing Before First Time Usage…………………….. …………..……………………………………

Set Up & Use…………………………………..…………………………………………………………

Trouble Shooting…………………………………………..……………………………………………

Technical Specifications……………………………………. …………..………………………………

Congratulations

You have just purchased a qualified baby monitor. Please read this instruction thoroughly before using and keep it for future reference.

Content and Features
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BABY UNIT
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1. Soft Antenna                                   5. Power OFF & Channel Switch 
2. Power Indicator                                 6. Belt clip
3. Mic                                                  7. Battery Compartment

4. Sensitivity Control

PARENTS UNIT
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Soft Antenna                               5. Power OFF & Channel Switch                
Sound & Power indicator                    6. Belt Clip         

3. Speaker                                   7. Battery Compartment
4. Volume Control                                                                 

Important!
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- This Baby Monitor is intended as an aid. Do not use it as a medical monitor or a 

substitute for responsible and proper adult supervision.

- Make sure the Baby Unit are out of child's reach. Do not place the Baby Unit inside the baby's crib or    playpen!

- The antenna on the Parents and Baby Units are fixed, do not try to extend them. Never 

attempt to modify the product.

Battery Installation

1. Locate the battery compartment door on the back of the Parents and Baby Units.

2. Open the battery compartment door.

3. Insert 3 AAA alkaline batteries into the Parents Unit & Baby Unit.

4. Replace battery compartment doors.
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Battery Tips:

- If the product is not in use for a long time, remove the batteries from both units.   
 otherwise battery leakage and corrosion can damage them.

- Dispose the batteries safely.

CAUTION: Danger of explosion if battery is incorrectly replaced. Dispose of used batteries according to the instructions. Replace only with the same or equivalent type. 

Testing Before First Time Usage

Test the Baby Unit transmission and the Parents Unit reception.

- Insert 3 AAA batteries into both units.
- Set both Parents and Baby Units to the same channel (1 or 2) by switching the channel switch.

-
Place Baby Unit in room where you intend to use it. Push the SENSITIVITY switch to Norm position to turn on the Baby Unit transmission. The power indicator lights (Please refer to Color Index of Power Indicator.)

-
Place Parents Unit in room where you intend to use it.

-
Light of sound level indicator lights when sound is received:

One or two dots light for shallow sound received.

Three or more dots light for louder sound received.

-
 When you experience interference (buzzing or static, etc.), switch both units to the alternative channel.

Color Index of Power Indicator

	 Color of   

       Power Indicator   

Power      

Sources
	Baby unit
	Parent unit

	Battery Operated (High Battery Level)
	Red
	Red

	Battery Operated (Low Battery Level)
	flashing
	flashing

	sound received (Baby unit & Parent Unit)
	
	stable


Set Up & Use
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IMPORTANT!  Test sound reception before use and whenever location of transmitter is changed. (Refer to Testing Before First Time Usage)

- Baby Unit detects sound levels within a range of  

1 to 2 meters (3 to 6.5 feet) for NORM setting.  

- Place Baby Unit in the same room with child. 

Place microphone directly toward child location,   

such as crib or playing area.

- Set both Parents and Baby units to the same 

channel (1 or 2)

- Push Baby Unit SENSITIVITY switch to NORM or 

HIGH position. The Power indicator lights (Please 

refer to Color Index of Power Indicator.)

- Adjust different detecting sound level sensitivity by switching the SENSITIVITY switch to 

either NORM (normal sensitivity: 1-2 meters) or HIGH (high sensitivity:2- 6 meters) position.

- The baby unit will go to stand-by mode for power saving when it doesn't detect sound from the surrounding area.    

- Place Parents Unit where you stay and hear it.

- Turn on the Parents Unit and change channel by rotating Power OFF & Channel Switch. Power indicator lights when the unit is on.(Please refer to Color Index of Power Indicator) 

- Rotate Volume dial of  parent unit to adjust volume.

Note:

Place the Baby Unit at least 1 meter away from the baby so that the microphone can pick up the child's sound.

Trouble shooting

	Problems
	Solutions

	1. No power
	- Unit is not turned on. Turn on the units. 

- Check if the batteries are installed properly. 

- The Unit may be battery low, change for new batteries.

	2.No power indicator

lights
	- Volume level on Parents Unit set too low. Adjust it to 

higher volume.

- Sound sensitivity level of Baby Unit is too low, Turn the 

Sound Sensitivity switch of Baby Unit to High position. 

- Units are out of range. Move Parents Unit closer to Baby Unit

- Ensure both units are in the same channel.

	3. Hearing static or 

Buzzing from Parents Unit
	- Make sure both units are set to the same channel

- Move the Parents Unit closer to the Baby Unit

Note: Communication range varies depending on surrounding conditions such as physical obstructions, interference.

- Reposition or replace batteries.

	4. Conversations or sounds from other homes received

	- Signal interference due to other nursery monitor on the 

same channel or cordless phone used. Change both units to another channel to eliminate source of interference.

	5. High pitched noise
	- The Parents and Baby Units are positioned too close to each 

other. Move Parents Unit away from Baby Unit.

- The volume is set too high. Lower the volume at the 

Parents Unit.


Technical Specifications

Power Supply Voltage:

Baby Unit-3 AAA alkaline batteries (not included)
Parent Unit-3 AAA alkaline batteries (not included)
Frequency: Channel 1: 49.860MHz       

          Channel 2: 49.890 MHz 
Channel:2 Channels

Operating Range: up to 100 meters

Set includes: 1 baby unit, 1 parent unit, 1 user manual.

CAUTION


This product cannot replace responsible adult supervision.


To reduce the risk of electric shock, do not expose this appliance to rain or moisture.









