
USER MANUAL
DIGITAL BABY MONITOR

MODEL: BM-175
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Congratulations 
You have just purchased a qualified Wireless 2.4GHz Digital Baby Monitor. Please read this instruction carefully before using the product. Keep these instructions for future reference.
Safety Precautions
When using this unit, basic Safety Precautions should always be followed to reduce the risk of fire, electric shock, or personal injury.
1. Read and understand all instructions.
2. Follow all warnings and instructions marked on this unit or mentioned in this operation instruction.
3. The outer surface of the Baby Unit and Parent Unit can be cleaned with a cloth LIGHTLY dampened with water or a mild cleaning solution.
4. Never put the system near water, such as bathtub, bathroom sink, laundry tub, kitchen sink or in a wet basement, etc. Immersion of this unit in water could cause an electrical shock.

5. Place the unit securely on a stable surface. Serious damage and/or injury may result if the unit falls.
6. Do not cover slots and openings on the unit. They are provided for ventilation and protection against overheating.
7. To reduce the risk of electric shock, do not disassemble this unit. Take the unit to authorized service center or qualified technician who service or repair work is required. Opening or removing covers may expose you to dangerous voltages or other risks. Incorrect reassembly can cause electric shock when the unit is subsequently used.
8. Do keep the system away from heat sources such as radiators, heat registers, stoves or other appliances producing heat. Also keep these components out of direct sunlight.
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Caution: 
This product cannot replace responsible adult supervision. 

1．This Baby Monitor is intended as an aid. Do not use it as a medical monitor or a substitute for responsible and proper adult supervision. 
2．Make sure the Parents unit and adaptor cable are always out of child's reach. Do not place the Baby Unit inside the baby's crib or playpen!

WARNING: 

-To reduce the risk of fire or electrical shock, do not expose this unit to rain or any type of moisture.
- This equipment should be installed and operated with minimum distance 20cm between the radiator & your baby。

Battery Tips:
（1） If the product is not in use for a long time, disconnect both units from the household electrical outlet. And remove the batteries or the exhausted batteries from the units, otherwise battery leakage and corrosion can damage them.
（2） Dispose the batteries safely.
Parents Unit：
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A. Name

①—Antenna            ②—LED audio indicator         ③—Power & Low battery indicator 

④—Speaker            ⑤—Volume Key                ⑥—Power ON/OFF/PAIR Key 

⑦—Belt Clip            ⑧—Hanging hook              ⑨—Battery Compartment

B. Operations Procedure

1. Power ON/OFF 

· Insert 3 AAA batteries.
· Turn the toggle switch⑥ to ON position and the power indicator③ will be green.

· Turn the toggle switch⑥ to OFF position and the power indicator③ will off

2. Pairing

· Turn the toggle switch⑥ of parents unit to PAIR position 

· Turn the toggle switch⑥ of baby unit to PAIR position

· Both the power indicator③ of parents unit and baby unit will slow flashing ，until a “BI” sound will be heard which means pairing successful，then enter normal mode automatically

    3. Volume Adjustment       

· Rotate the knob switch⑤ up，the volume level will increasing until highest

· Rotate the knob switch⑤ down，the volume level will decreasing until lowest


4. Low Battery Indicator
· When the unit is in low battery, the power indicator③ will be quick flashing which means the battery is low.
· The unit will be powered off when voltage is lower than 3.0V.
5. Out of Range Alert (Only for Parents unit)

The parents unit will give out “BI, BI” sound alert and the five LED audio indicator② will slow flashing at the same time which will be appeared under such circumstances.
· The units are detected out of communication range.
· One of the parents and baby unit is in low battery or turned off.
Remark: LED audio indicator② will be changing as per the received sound volume.

Baby Unit
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A. Name

①—Antenna          ②—Power & Low battery indicator          ③—Microphone 

④—Volume Key       ⑤—Power ON/OFF/PAIR Key             ⑥—Belt Clip

⑦—Hanging hook      ⑧—Battery Compartment             

B. Operations Procedure

1. Power ON/OFF 

· Insert 3 AAA batteries.
· Turn the toggle switch⑤ to ON position and the power indicator③ will be green.

· Turn the toggle switch⑤ to OFF position and the power indicator③ will off

2. Pairing

· Turn the toggle switch⑤ of parents unit to PAIR position 

· Turn the toggle switch⑤ of baby unit to PAIR position

· Both the power indicator③ of parents unit and baby unit will slow flashing ，until a “BI” sound will be heard which means pairing successful，then enter normal mode automatically 

    3. Volume Adjustment       

· Rotate the knob switch④ up，the volume level will increasing until highest

· Rotate the knob switch④ down，the volume level will decreasing until lowest


4. Low Battery Indicator
· When the unit is in low battery, the power indicator② will be quick flashing which means the battery is low.
· The unit will be powered off when voltage is lower than 3.0V.
Remark: LED audio indicator will be changing as per the received sound volume.

5. Communication.

· Parent unit can receive the sound from baby unit when baby sound reaches 60dB.

Trouble shooting 

	Problems
	Solutions

	1. No power
	- Unit is turned off. 

- Check if the batteries are installed properly. 

- The Unit may be in low battery status, change new batteries.

	2. Message not 

transmitted.



	-  Volume level of Baby unit is too low, Rotate the knob switch to HI level.

- Units are out of range or lost connection. Ensure the distance between the units within communication range. 

Note: Communication range varies depending on surrounding 

conditions such as physical obstructions, interference.

- Ensure both units have already scanned the corresponding  

code.

	3. No sound signal
	- Volume level on Parents unit is set too low. Adjust it to higher volume.

- Volume level on Baby unit is too low, the Rotate the knob switch to HI level.                              

- Units are out of range. Ensure the distance between the units within communication range.

- Ensure both units toggle switch on the same position，all on ON position or all on PAIR position

	4. Received 

Conversation or 

sound from neighbors.

	- Signal interference due to other nursery monitor on the same ID Code or cordless phone used.

- Operate "Code Pairing" Again.

	5. Hearing static or rustle from Parent unit.
	- The both units are positioned too close to each other. Keep away two units at about 1m.

- The volume is set too high. Lower the volume at the Parent unit.

- Reposition or replace batteries.

	6. Power LED rapidly flashes green light and can not receive or transmit 
	- The power is too low. Replace the new batteries
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THIS PRODUCT COMPLIES WITH EU DIRECTIVE 2012/19/EC.

The crossed bin symbol on the appliance indicates that the product, at the end of its life, must be disposed of separately from domestic waste, either by taking it to a separate waste disposal site for electric and electronic appliances or by returning it to your dealer when you buy another similar appliance. The user is responsible for taking the appliance to a special waste disposal site at the end of its life. If the end-of-life product is collected correctly as separate waste , it can be recycled, processed and disposed of ecologically ; this avoids a negative impact on both the environment and human health , and contributes towards the recycling of the product’s materials. For further information regarding the waste disposal services available, contact your local waste disposal agency or the shop where you bought the appliance.

Declaration of compliance
Hereby,  declares that the radio equipment type BM-175 is in compliance with Directive 2014/53/EU. 

The full text of the EU declaration of conformity is available at the following internet address: 
Symbols key
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 Complies with relevant EC directives as amended
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Warning!

Technical Specifications
Adaptor voltage: 5V 1A (adaptor x 2)

Work temperature：0-40℃
Transmitter – 3 AAA alkaline batteries  (not included) or supplied adaptor 
Receiver   – 3 AAA alkaline batteries  (not included) or supplied adaptor 
Operation Frequency:  2.40-2.4835GHz

Transmission power<20dbm                                                             

Operating Range: up to 300 metre in ideal conditions

Set include:  1 baby unit, 1 parent unit. 2 adaptors
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